<?xml version="1.0" encoding="UTF-8"?>
<!DOCTYPE datafile PUBLIC "-//Logiqx//DTD ROM Management Datafile//EN" "http://www.logiqx.com/Dats/datafile.dtd">

<datafile>
	<header>
		<name>MAME BIOS</name>
		<description>MAME BIOS 0.274</description>
		<category>Emulation</category>
		<version>0.274</version>
		<date>31/01/2025</date>
		<author>AntoPISA</author>
		<homepage>https://www.progettosnaps.net/</homepage>
		<url>https://www.progettosnaps.net/dats/MAME/</url>
		<clrmamepro/>
	</header>
	<machine name="3dobios" sourcefile="misc/3do.cpp" isbios="yes" runnable="no">
		<description>3DO BIOS</description>
		<year>1993</year>
		<manufacturer>The 3DO Company</manufacturer>
		<biosset name="panafz10" description="Panasonic FZ-10 R.E.A.L. 3DO Interactive Multiplayer"/>
		<biosset name="goldstar" description="Goldstar 3DO Interactive Multiplayer v1.01m"/>
		<biosset name="panafz1" description="Panasonic FZ-1 R.E.A.L. 3DO Interactive Multiplayer"/>
		<biosset name="sanyotry" description="Sanyo TRY 3DO Interactive Multiplayer"/>
		<rom name="goldstar.bin" size="1048576" crc="b6f5028b" sha1="c4a2e5336f77fb5f743de1eea2cda43675ee2de7"/>
		<rom name="panafz1.bin" size="1048576" crc="c8c8ff89" sha1="34bf189111295f74d7b7dfc1f304d98b8d36325a"/>
		<rom name="panafz10.bin" size="1048576" crc="58242cee" sha1="3c912300775d1ad730dc35757e279c274c0acaad"/>
		<rom name="sanyotry.bin" size="1048576" crc="d5cbc509" sha1="b01c53da256dde43ffec4ad3fc3adfa8d635e943"/>
		<device_ref name="arm7_be"/>
		<device_ref name="nvram"/>
		<device_ref name="timer"/>
		<device_ref name="screen"/>
		<device_ref name="cdrom_image"/>
	</machine>
	<machine name="airlbios" sourcefile="sega/naomi.cpp" isbios="yes" runnable="no">
		<description>NAOMI Airline Pilots (deluxe) BIOS</description>
		<year>1999</year>
		<manufacturer>Sega</manufacturer>
		<biosset name="bios0" description="Airline Pilots Deluxe (Export)"/>
		<biosset name="bios1" description="Airline Pilots Deluxe (USA)"/>
		<rom name="epr-21801.ic27" size="2097152" crc="a21bef24" sha1="c6c6ed09772b63a9a84ef0678fc1b7527484038a"/>
		<rom name="epr-21802.ic27" size="2097152" crc="a77c6b1c" sha1="bd50a6bb8fa9bac121b076e21ea048a83a240a48"/>
		<rom name="main_eeprom.bin" size="128" crc="fea29cbb" sha1="4099f1747aafa07db34f6e072cd9bfaa83bae10e"/>
		<rom name="x76f100_eeprom.bin" size="132" crc="3ea24b6a" sha1="3a730ebcf56e0060fef6b1b02eb2eb7cfb7e61dc"/>
		<device_ref name="sh4le"/>
		<device_ref name="timer"/>
		<device_ref name="dc_g2if"/>
		<device_ref name="arm7_le"/>
		<device_ref name="maple_dc"/>
		<device_ref name="screen"/>
		<device_ref name="powervr2"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="aica"/>
		<device_ref name="aicartc"/>
		<device_ref name="93c46_16"/>
		<device_ref name="mie"/>
		<device_ref name="z80"/>
		<device_ref name="mie_jvs"/>
		<device_ref name="jvs13551"/>
		<device_ref name="tmp90ph44"/>
		<device_ref name="93c46_8"/>
		<device_ref name="x76f100"/>
		<device_ref name="m3comm"/>
		<device_ref name="m68000"/>
		<device_ref name="ram"/>
		<device_ref name="nvram"/>
		<device_ref name="naomi_rom_board"/>
	</machine>
	<machine name="aleck64" sourcefile="nintendo/aleck64.cpp" isbios="yes" runnable="no">
		<description>Aleck64 PIF BIOS</description>
		<year>1998</year>
		<manufacturer>Nintendo / Seta</manufacturer>
		<rom name="normpnt.rom" size="128" crc="e7f2a005" sha1="c27b4a364a24daeee6e99fd286753fd6216362b4"/>
		<rom name="normslp.rom" size="128" crc="4f2ae525" sha1="eab43f8cc52c8551d9cff6fced18ef80eaba6f05"/>
		<rom name="pifdata.bin" size="2048" crc="5ec82be9" sha1="9174eadc0f0ea2654c95fd941406ab46b9dc9bdd"/>
		<device_ref name="vr4300be"/>
		<device_ref name="rsp"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="dmadac"/>
		<device_ref name="dmadac"/>
		<device_ref name="n64_periphs"/>
	</machine>
	<machine name="alg3do" sourcefile="misc/3do.cpp" isbios="yes" runnable="no">
		<description>ALG 3DO BIOS</description>
		<year>1993</year>
		<manufacturer>American Laser Games / The 3DO Company</manufacturer>
		<rom name="saot_rom2.bin" size="524288" crc="b832da9a" sha1="520d3d1b5897800af47f92efd2444a26b7a7dead"/>
		<device_ref name="arm7_be"/>
		<device_ref name="nvram"/>
		<device_ref name="timer"/>
		<device_ref name="screen"/>
		<device_ref name="cdrom_image"/>
	</machine>
	<machine name="alg_bios" sourcefile="amiga/alg.cpp" isbios="yes" runnable="no">
		<description>American Laser Games BIOS</description>
		<year>199?</year>
		<manufacturer>American Laser Games</manufacturer>
		<biosset name="kick13" description="Kickstart 1.3 (34.5)"/>
		<rom name="315093-02.u2" size="262144" crc="c4f0f55f" sha1="891e9a547772fe0c6c19b610baf8bc4ea7fcb785"/>
		<device_ref name="m68000"/>
		<device_ref name="address_map_bank"/>
		<device_ref name="address_map_bank"/>
		<device_ref name="nvram"/>
		<device_ref name="screen"/>
		<device_ref name="agnus_copper"/>
		<device_ref name="ldp1450"/>
		<device_ref name="palette"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="paula_8364"/>
		<device_ref name="mos8520"/>
		<device_ref name="mos8520"/>
		<device_ref name="paula_fdc"/>
	</machine>
	<machine name="allied" sourcefile="pinball/allied.cpp" sampleof="genpin" isbios="yes" runnable="no">
		<description>Allied System</description>
		<year>1977</year>
		<manufacturer>Allied Leisure</manufacturer>
		<rom name="6530-009.u5" size="1024" crc="e4fb64fb" sha1="a3d9de7cbfb42180a860e0bbbeaeba96d8bd1e20"/>
		<rom name="6530-010.u6" size="1024" crc="dca980dd" sha1="3817d75413854d889fc1ce4fd6a51d820d1e0534"/>
		<rom name="6530-011.u3" size="1024" crc="13f42789" sha1="baa0f73fda08a3c5d6f1423fb329e4febb07ef97"/>
		<device_ref name="m6504"/>
		<device_ref name="ipt_merge_any_hi"/>
		<device_ref name="speaker"/>
		<device_ref name="samples"/>
		<device_ref name="pia6821"/>
		<device_ref name="pia6821"/>
		<device_ref name="pia6821"/>
		<device_ref name="pia6821"/>
		<device_ref name="pia6821"/>
		<device_ref name="mos6530"/>
		<device_ref name="mos6530"/>
		<device_ref name="mos6530"/>
		<device_ref name="timer"/>
		<sample name="bumper"/>
		<sample name="chime1"/>
		<sample name="chime2"/>
		<sample name="chime3"/>
		<sample name="chime4"/>
		<sample name="coil_coinlockout_engage"/>
		<sample name="coil_coinlockout_release"/>
		<sample name="coinin"/>
		<sample name="drop_target_reset"/>
		<sample name="hole"/>
		<sample name="kickback"/>
		<sample name="knocker"/>
		<sample name="outhole"/>
		<sample name="relay_engage"/>
		<sample name="relay_release"/>
		<sample name="sling"/>
		<sample name="solenoid_engage"/>
		<sample name="solenoid_release"/>
	</machine>
	<machine name="ar_bios" sourcefile="amiga/arsystems.cpp" isbios="yes" runnable="no">
		<description>Arcadia System BIOS</description>
		<year>1988</year>
		<manufacturer>Arcadia Systems</manufacturer>
		<biosset name="onep300" description="OnePlay 3.00"/>
		<biosset name="onep220" description="OnePlay 2.20"/>
		<biosset name="onep211" description="OnePlay 2.11"/>
		<biosset name="tenp211" description="TenPlay 2.11"/>
		<biosset name="tenp311" description="TenPlay 3.11"/>
		<biosset name="tenp400" description="TenPlay 4.00"/>
		<rom name="315093-01.u2" size="262144" crc="a6ce1636" sha1="11f9e62cf299f72184835b7b2a70a16333fc0d88"/>
		<rom name="gcp-1-hi" size="65536" crc="67d44523" sha1="f3e3699132cdf741518accb890c04d17374c4049"/>
		<rom name="gcp-1-lo" size="65536" crc="65d9b9cf" sha1="5c60a0dd4a0a7d9b938ce6b0446a6ad2ecaf07ec"/>
		<rom name="gcp-2-hi" size="65536" crc="1d7594ae" sha1="6173bbfecf18d7d9ee6bc2b6753ca9d42fabd781"/>
		<rom name="gcp-2-lo" size="65536" crc="e776198d" sha1="694ca4cc99ed84a95d18201c94a3332f8599654f"/>
		<rom name="gcp-3-hi" size="65536" crc="3e7364be" sha1="26e10d0ddc031a891138db36ce4f1732722e6847"/>
		<rom name="gcp-3-lo" size="65536" crc="87229e0d" sha1="0b18544801e529f954b9e03226bd2e5475f36351"/>
		<rom name="gcp_v311_1-hi.u16" size="65536" crc="0b486a85" sha1="b406f1db5abf28d9072b7940989ffd176aeee5cb"/>
		<rom name="gcp_v311_1-lo.u11" size="65536" crc="80e8e863" sha1="ab04dfcda7544f4ed9b67771cd8aefe0300c6d4b"/>
		<rom name="gcp_v311_2-hi.u17" size="65536" crc="d20a4d7f" sha1="1dc0a79efa946333149f68ddac046fd44b5f2abe"/>
		<rom name="gcp_v311_2-lo.u12" size="65536" crc="5bf4c74c" sha1="1f7b17170accdf9e448c1a5d8bc430aa2d1d931b"/>
		<rom name="gcp_v400_1-hi.u16" size="65536" crc="69295167" sha1="855f53abbb9dc15e5518e16c5c2dfe4134d07306"/>
		<rom name="gcp_v400_1-lo.u11" size="65536" crc="504c2171" sha1="a93367f520afb86c97c0a191714b72823c95cdd2"/>
		<rom name="gcp_v400_2-hi.u17" size="65536" crc="13fb4e2d" sha1="3eef07aecc3a201ae0b20634c7fd0c87c89fd7f1"/>
		<rom name="gcp_v400_2-lo.u12" size="65536" crc="a5cc4515" sha1="80070521476e92323a6baa6e55928ca5b751a332"/>
		<rom name="scpa_01-hi_v2.11.u12" size="65536" crc="be9dbdc5" sha1="1554da09f051ec53937d65d4e451de51bc0c69e5"/>
		<rom name="scpa_01-hi_v2.20.u12" size="65536" crc="79450b4b" sha1="a1e508a89fc62e1c4994064f2786f491b1dc8bc6"/>
		<rom name="scpa_01-hi_v3.0.u12" size="65536" crc="2d8e1a06" sha1="be187f34624aeda110017c4a09242f7c00ef56a4"/>
		<rom name="scpa_01-lo_v2.11.u16" size="65536" crc="95b84504" sha1="99999fc40909001b37aa1b543918118becc81800"/>
		<rom name="scpa_01-lo_v2.20.u16" size="65536" crc="d2825511" sha1="747a37c6073224472bf261ae376ac9abfbe07554"/>
		<rom name="scpa_01-lo_v3.0.u16" size="65536" crc="e4f38fab" sha1="01c2eb5965070893be6734eb1372576727716476"/>
		<device_ref name="m68000"/>
		<device_ref name="address_map_bank"/>
		<device_ref name="address_map_bank"/>
		<device_ref name="agnus_copper"/>
		<device_ref name="nvram"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="paula_8364"/>
		<device_ref name="mos8520"/>
		<device_ref name="mos8520"/>
		<device_ref name="paula_fdc"/>
	</machine>
	<machine name="aristmk5" sourcefile="acorn/aristmk5.cpp" isbios="yes" runnable="no">
		<description>MKV Set-Clear Chips (US)</description>
		<year>1995</year>
		<manufacturer>Aristocrat</manufacturer>
		<rom name="a562837.u36" size="343" crc="1f269234" sha1="29940dd50fb55c632935f62ff44ca724379c7a43"/>
		<rom name="a562838.u65" size="343" crc="f2f3c40a" sha1="b795dfa5cc4e8127c3f3a0906664910d1325ec92"/>
		<rom name="a562840.u22" size="343" crc="941d4cdb" sha1="1ca091fba69e92f262dbb3d40f515703c8981793"/>
		<rom name="clear_mk5_u_11_ck_3a6f.u11" size="524288" crc="4cf70173" sha1="f3dda0f188c035a36954048b449b9b96787709f2"/>
		<rom name="clear_mk5_u_7_ck_eb68.u7" size="524288" crc="e8e8dc75" sha1="201fe95256459ce34fdb6f7498135ab5016d07f3"/>
		<rom name="setchip v1.0.u11" size="524288" crc="a969f12b" sha1="fc6d234ce1f5c6b5aceb97b73aad60144352023b"/>
		<rom name="setchip v1.0.u7" size="524288" crc="16c2828d" sha1="87218a76bb2791bce27b4b8ab341ba73cbbf6ffe"/>
		<rom name="setchip v4.02.04.u11" size="524288" crc="def36617" sha1="c7ba5b08e884a8fb36c9fb51c08e243e32c81f89"/>
		<rom name="setchip v4.02.04.u7" size="524288" crc="5a254b22" sha1="8444f237b392df2a3cb42ea349e7af32f47dd544"/>
		<rom name="setchip v4.02.04_alt.u11" size="524288" crc="254e8b03" sha1="0ed9723258d3f86b21bf132cbe2fd0bae978cd5e"/>
		<rom name="setchip v4.02.04_alt.u7" size="524288" crc="41275334" sha1="d4a63dbc77c2c44f6a9c72b389bd270f2137997f"/>
		<rom name="setchip v4.03.07.u11" size="524288" crc="637de9b9" sha1="4b5c974fd4c1d1a21f83bdc03d8bc5013d4a40ea"/>
		<rom name="setchip v4.03.07.u7" size="524288" crc="5cf56036" sha1="ff11deb6f76627f4fb5a7ec789e4071887e3eae9"/>
		<rom name="setchip v4.04.00.u11" size="524288" crc="82dfa12a" sha1="86fd0f0ad8d5d1bc503392a40bbcdadb055b2765"/>
		<rom name="setchip v4.04.00.u7" size="524288" crc="2453137e" sha1="b59998e75ae3924da16faf47b9cfe9afd60d810c"/>
		<rom name="setchip v4.04.01 cs 1358.u7" size="524288" crc="1d564c2c" sha1="2e47917138c682393a61676da6fccba90463229a" status="baddump"/>
		<rom name="setchip v4.04.01 cs ed54.u11" size="524288" crc="199bacff" sha1="a2ef556b42d505af077a2db983caebdd611d98fd"/>
		<rom name="setchip v4.04.05.u11" size="524288" crc="2fc9b2a0" sha1="89191f02c4ec8089e26989430806650d14e13e5a"/>
		<rom name="setchip v4.04.05.u7" size="524288" crc="e7b39a73" sha1="e826d717a0871383394e15634896fcb2e2bdeb75"/>
		<rom name="setchip v4.04.08.u11" size="524288" crc="d3234a28" sha1="8ff112ee4aadf1d359ca8ffe0cfa9c7400aa0595"/>
		<rom name="setchip v4.04.08.u7" size="524288" crc="7c4b7fe4" sha1="39dd39c794c0cb6abc1b7503650643a8131468d1"/>
		<rom name="setchip v4.04.09.u11" size="524288" crc="ff7a9035" sha1="4352c4336e61947c555fdc80c61f944076f64b64"/>
		<rom name="setchip v4.04.09.u7" size="524288" crc="e8e8dc75" sha1="201fe95256459ce34fdb6f7498135ab5016d07f3"/>
		<device_ref name="arm_cpu"/>
		<device_ref name="watchdog"/>
		<device_ref name="memc"/>
		<device_ref name="ioc"/>
		<device_ref name="screen"/>
		<device_ref name="acorn_vidc1a"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="dac_16bit_r2r_tc"/>
		<device_ref name="dac_16bit_r2r_tc"/>
		<device_ref name="dac_16bit_r2r_tc"/>
		<device_ref name="dac_16bit_r2r_tc"/>
		<device_ref name="dac_16bit_r2r_tc"/>
		<device_ref name="dac_16bit_r2r_tc"/>
		<device_ref name="dac_16bit_r2r_tc"/>
		<device_ref name="dac_16bit_r2r_tc"/>
		<device_ref name="93c56_16"/>
		<device_ref name="93c56_16"/>
		<device_ref name="nvram"/>
		<device_ref name="ns16450"/>
		<device_ref name="ns16450"/>
		<device_ref name="ns16450"/>
		<device_ref name="ns16450"/>
		<device_ref name="ns16450"/>
		<device_ref name="ns16450"/>
		<device_ref name="ns16450"/>
		<device_ref name="ns16450"/>
		<device_ref name="ipt_merge_any_hi"/>
		<device_ref name="ds1302"/>
		<device_ref name="coin_hopper"/>
		<device_ref name="rs232"/>
	</machine>
	<machine name="aristmk6" sourcefile="aristocrat/aristmk6.cpp" isbios="yes" runnable="no">
		<description>MK6 System Software-Setchips</description>
		<year>2000</year>
		<manufacturer>Aristocrat</manufacturer>
		<biosset name="au-nsw1" description="Aristocrat MK6 Base (24013001, NSW/ACT)"/>
		<biosset name="au-nsw2" description="Aristocrat MK6 Base (21012901, NSW/ACT)"/>
		<biosset name="au-nsw3" description="Aristocrat MK6 Base (19012801, NSW/ACT)"/>
		<biosset name="au-nsw4" description="Aristocrat MK6 Base (13012001, NSW/ACT)"/>
		<biosset name="au-nsw5" description="Aristocrat MK6 Base (11011901, NSW/ACT)"/>
		<biosset name="au-nsw6" description="Aristocrat MK6 Base (11011501, NSW/ACT)"/>
		<biosset name="au-nsw7" description="Aristocrat MK6 Base (09011001, NSW/ACT)"/>
		<biosset name="au-nsw8" description="Aristocrat MK6 Base (07010801, NSW/ACT)"/>
		<biosset name="au-nsw9" description="Aristocrat MK6 Base (05010601, NSW/ACT)"/>
		<biosset name="au-nsw10" description="Aristocrat MK6 Base (04010501, NSW/ACT)"/>
		<biosset name="au-nsw11" description="Aristocrat MK6 Base (03010301, NSW/ACT)"/>
		<biosset name="au-nsw12" description="Aristocrat MK6 Base (02010201, NSW/ACT)"/>
		<biosset name="au-nsw13" description="Aristocrat MK6 Base (02010114, NSW/ACT)"/>
		<biosset name="au-qld1" description="Aristocrat MK6 Base (25012805, Queensland)"/>
		<biosset name="au-qld2" description="Aristocrat MK6 Base (20012605, Queensland)"/>
		<biosset name="au-qld3" description="Aristocrat MK6 Base (20012305, Queensland)"/>
		<biosset name="au-qld4" description="Aristocrat MK6 Base (14011605, Queensland)"/>
		<biosset name="au-qld5" description="Aristocrat MK6 Base (04041205, Queensland)"/>
		<biosset name="au-qld6" description="Aristocrat MK6 Base (03130334, Queensland)"/>
		<biosset name="au-qld7" description="Aristocrat MK6 Base (01040505, Queensland)"/>
		<biosset name="au-sa1" description="Aristocrat MK6 Base (03030708, South Australia)"/>
		<biosset name="nz1" description="Aristocrat MK6 Base (14011913, New Zealand)"/>
		<biosset name="nz2" description="Aristocrat MK6 Base (14010152, New Zealand)"/>
		<biosset name="nz3" description="Aristocrat MK6 Base (02061013, New Zealand)"/>
		<biosset name="nz4" description="Aristocrat MK6 Base (02060913, New Zealand)"/>
		<biosset name="my" description="Aristocrat MK6 Base (15011025, Malaysia)"/>
		<biosset name="afr" description="Aristocrat MK6 Base (24010467, Africa)"/>
		<biosset name="us1" description="Aristocrat MK6 Base (01.04.11, US)"/>
		<biosset name="us2" description="Aristocrat MK6 Base (01.04.10, US)"/>
		<biosset name="us3" description="Aristocrat MK6 Base (01.04.08, US)"/>
		<biosset name="us4" description="Aristocrat MK6 Base (01.04.07, US)"/>
		<biosset name="us5" description="Aristocrat MK6 Base (01.04.04, US)"/>
		<biosset name="us6" description="Aristocrat MK6 Base (01.03.17, US)"/>
		<biosset name="us7" description="Aristocrat MK6 Base (01.03.14, US)"/>
		<biosset name="us8" description="Aristocrat MK6 Base (01.03.07, US)"/>
		<biosset name="us9" description="Aristocrat MK6 Base (01.03.06, US)"/>
		<biosset name="us10" description="Aristocrat MK6 Base (01.03.05, US)"/>
		<biosset name="us11" description="Aristocrat MK6 Base (01.03.03e, US)"/>
		<biosset name="us12" description="Aristocrat MK6 Base (01.03.03a, US)"/>
		<biosset name="us13" description="Aristocrat MK6 Base (01.02.08, US)"/>
		<biosset name="us14" description="Aristocrat MK6 Base (01.02.02, US)"/>
		<biosset name="set-us1" description="Aristocrat MK6 Set Chips (06.03.04, US)"/>
		<biosset name="set-us2" description="Aristocrat MK6 Set Chips (06.03.03, US)"/>
		<biosset name="set-us3" description="Aristocrat MK6 Set Chips (06.02.20, US)"/>
		<biosset name="set-us4" description="Aristocrat MK6 Set Chips (06.02.04, US)"/>
		<rom name="01.02.02_left.u3" size="1048576" crc="1d0f4093" sha1="17d6328dba9826b58f39393ca2f2daac1b7161ef"/>
		<rom name="01.02.02_right.u2" size="1048576" crc="e920e940" sha1="52e28d4765a3e953bb70dc4ed13d96d4180be996"/>
		<rom name="01.02.08_left.u3" size="1048576" crc="f29fd1bf" sha1="33e043d2616e10a1c7a0936c3d208f9bcc2ca6f3"/>
		<rom name="01.02.08_right.u2" size="1048576" crc="aaaeac8c" sha1="a565e5fcb4f55f31e7d36be40eec234248a66efd"/>
		<rom name="01.03.03a_left.u70" size="2097152" crc="4ab5dd40" sha1="a6812cc624e6a98ea7b0697e2797fe10ba8e303e"/>
		<rom name="01.03.03a_right.u83" size="2097152" crc="253415f4" sha1="50dc77ad87bc6be1932dda2fd4865602c8c49729"/>
		<rom name="01.03.03e_left.u70" size="2097152" crc="ea50729a" sha1="14b5a71bfb91ac366ddcb5f77fb54127808f8163"/>
		<rom name="01.03.03e_right.u83" size="2097152" crc="2255e263" sha1="5e9e093aaa17172f47a14c3baf7f6f0f73b19398"/>
		<rom name="01.03.05_left.u70" size="2097152" crc="0095e3f9" sha1="d2e8786158b1ab0a614aab21cf1d14cbc04754af"/>
		<rom name="01.03.05_right.u83" size="2097152" crc="2c7f1ec3" sha1="d03167f43ed6f9596080d91472695829378cef0a"/>
		<rom name="01.03.06_left.u70" size="2097152" crc="2f9d9a29" sha1="fdebfaca9a579d7249379f19aef22fbfd66bf943"/>
		<rom name="01.03.06_right.u83" size="2097152" crc="bd48ca55" sha1="8fb1576cbeb1c64c358880714740195d2e73e03e"/>
		<rom name="01.03.07_left.u70" size="2097152" crc="a3632da4" sha1="1c96a88e86095b81801ab88e36a4cdfa4b893265"/>
		<rom name="01.03.07_right.u83" size="2097152" crc="2ebccc4e" sha1="9342724e4451e9ab24ceae208284b50abd4f0be3"/>
		<rom name="01.03.14_left.u70" size="2097152" crc="7138fec4" sha1="f81331d1875ac574d3e6c98be218ff25c6c7be5a"/>
		<rom name="01.03.14_right.u83" size="2097152" crc="889ffd82" sha1="9c98c9cdcf5f7d05095f11006418133029e9f0f8"/>
		<rom name="01.03.17_left.u70" size="2097152" crc="a88193dc" sha1="c9e1d483edaecd318d2e5fc8a54e84516c93e0ca"/>
		<rom name="01.03.17_right.u83" size="2097152" crc="1582714b" sha1="92d0a15314ffe526159bef9a364898dd1ebdfde7"/>
		<rom name="01.04.04_left.u70" size="2097152" crc="b984a92c" sha1="90f7a61302caee40195c08565bdac856a3234c1d"/>
		<rom name="01.04.04_right.u83" size="2097152" crc="e57ba02d" sha1="8e29403e6b619eeab41dc171221720bc7820ccdc"/>
		<rom name="01.04.07_left.u70" size="2097152" crc="acfb0fe0" sha1="b1a772d7978e6ff4406a5bb39a71cb3f89608e72"/>
		<rom name="01.04.07_right.u83" size="2097152" crc="23c28e22" sha1="98f24a1f86232b6c2c288a61ec7d60c867f192e5"/>
		<rom name="01.04.08_left.u70" size="2097152" crc="0dfcad10" sha1="53798be000304aed38909f5fd8470a68bedd8229"/>
		<rom name="01.04.08_right.u83" size="2097152" crc="95333304" sha1="7afe49d6c5e4d6820f349778557daa88c5366a51"/>
		<rom name="01.04.10_left.u70" size="2097152" crc="9d9d52c1" sha1="b957220cdbedd516c219d1bfc28807ce466df93f"/>
		<rom name="01.04.10_right.u83" size="2097152" crc="82ce2fcc" sha1="4c8fb3db084a67e99d1420b3f895a06ce9ef5ec2"/>
		<rom name="01.04.11_left.u70" size="2097152" crc="787f2b07" sha1="2548289e44f4b935346b759afb5383bdbac04c3e"/>
		<rom name="01.04.11_right.u83" size="2097152" crc="2dae8ca0" sha1="7a0fb38b4c1ac7195d15bdab6f0cfb16c78430f0"/>
		<rom name="01040505.u70" size="1048576" crc="b9ddea66" sha1="f4bfdeada39a3f0094d6468b7374a34f88f5df7f"/>
		<rom name="01040505.u71" size="1048576" crc="f56ea77e" sha1="319be1bee66a289e2c1f6beec07758f79aa0cf16"/>
		<rom name="01040505.u83" size="1048576" crc="90f32169" sha1="228be8b4a9eb6b2acf7f7a7561bd194009936026"/>
		<rom name="01040505.u84" size="1048576" crc="cf5a9d1e" sha1="0ebba478fc883831d70b0fa95f43e5f93b07ae9e"/>
		<rom name="02010114.u70" size="1048576" crc="3ba4379f" sha1="84367f12c4c9224d2ab9cae83ae8727de338408c"/>
		<rom name="02010114.u71" size="1048576" crc="8f83c3dd" sha1="a5f9d80b4b515b24299d0241e1665cfd9da8bab7"/>
		<rom name="02010114.u83" size="1048576" crc="945104d7" sha1="e372d0cf889c72b5d001b26fe4a925a28486537f"/>
		<rom name="02010114.u84" size="1048576" crc="183e3836" sha1="4c802d0cd010bc007acb3a83e37aaa29b2d13d87"/>
		<rom name="02010201.u70" size="1048576" crc="9b2db442" sha1="d512398a2d9257bd385dc50d61c63cd1a47300ba"/>
		<rom name="02010201.u71" size="1048576" crc="24d5614a" sha1="fdcf3826dccc72b74b66379b1411cf211d5a1670"/>
		<rom name="02010201.u83" size="1048576" crc="5f64a20c" sha1="397404ab6d2a1aa3c1fc77bb9421fef7079b65a5"/>
		<rom name="02010201.u84" size="1048576" crc="0920930f" sha1="771b0f62442d1c75b1bb59ad82365b7ab8747173"/>
		<rom name="02060913_left.u70" size="1048576" crc="d6a6713c" sha1="0f3bb2746f1a6fa6a587fd50827299408a3b28d2"/>
		<rom name="02060913_right.u83" size="1048576" crc="31068c41" sha1="962da0079495a64f7ffb34be643892c272017cc9"/>
		<rom name="02061013_left.u70" size="1048576" crc="e70a7007" sha1="0935f924866162d9c0fbdbb99391cbf730a04b76"/>
		<rom name="02061013_right.u83" size="1048576" crc="7a8619a5" sha1="bd03ddb68817c1660b009e102ccf69e5b603b875"/>
		<rom name="03010301.u70" size="1048576" crc="5ae69121" sha1="36dd3f9aaf5f7d2751d1954d67f898bc3ec71f3b"/>
		<rom name="03010301.u71" size="1048576" crc="d793440a" sha1="dced4c04bde13293af77a9a1f4c5c606e3758de0"/>
		<rom name="03010301.u83" size="1048576" crc="c8580554" sha1="58b8bfff2f8d298c4e3be2b01900800c45fa7ad7"/>
		<rom name="03010301.u84" size="1048576" crc="a34a9f16" sha1="b8750e6ceb1715da8e5ac2f0183254e29a042641"/>
		<rom name="03030708_left.u70" size="1048576" crc="4e5ad823" sha1="77ab1c29c6172cfdcef776222a72b2b44114d4da"/>
		<rom name="03030708_right.u83" size="1048576" crc="b4b3c6a5" sha1="5747f98a6eaa5c24a23d1d76a28b33a3bfbbfd1f"/>
		<rom name="03130334_left.u70" size="2097152" crc="02175fde" sha1="4e9a9e1e803a0c84b06aec99dc3147dd7a919eee"/>
		<rom name="03130334_right.u83" size="2097152" crc="bce3d97f" sha1="da36377cc1465022a2434703adee63bf48c71a9c"/>
		<rom name="04010501_left.u70" size="1048576" crc="21182775" sha1="7c5b7f5aba3babc85f512a8f7d4ebc0d83eb842a"/>
		<rom name="04010501_right.u83" size="1048576" crc="3daefb7a" sha1="411471713219f4bab5ccf5fe7a12a6c138c8c550"/>
		<rom name="04041205_left.u70" size="1048576" crc="dfb9a119" sha1="814a5a7877392aec4e4871d7f0e19d2fbd717409"/>
		<rom name="04041205_right.u83" size="1048576" crc="ca6bc86c" sha1="69fe7fc35694e4cd7f861bff4ec3a6165a81df6e"/>
		<rom name="05010601_left.u70" size="1048576" crc="b3e6b4a0" sha1="3bf398c9257579f8e51ce716d6ebfa74fa510273"/>
		<rom name="05010601_right.u83" size="1048576" crc="c12eac11" sha1="683b9ddc323865ace7dca37d13b55de6e42759a5"/>
		<rom name="06.02.04_left.u3" size="1048576" crc="117b75f2" sha1="2129286853d3c50b8a943b71334d4ef6b98adc05"/>
		<rom name="06.02.04_right.u2" size="1048576" crc="1cf5a853" sha1="64d17efcce702df7a0b0e151293199478e25226d"/>
		<rom name="06.02.20_left.u70" size="1048576" crc="199ed3b9" sha1="e3ee81ffd713f09e35a10c38e4f59282e2c5cd30"/>
		<rom name="06.02.20_right.u83" size="1048576" crc="e4001f60" sha1="5da34efb1ac0f7c84a48e09363d20cfecda4bcf1"/>
		<rom name="06.03.03_left.u3" size="1048576" crc="a6924238" sha1="b71ab39bf9c1fdbab556028138749e8c040ec83c"/>
		<rom name="06.03.03_right.u2" size="1048576" crc="98763498" sha1="246e95cc12eb34f946b2f4938c59217718f6d841"/>
		<rom name="06.03.04_left.u3" size="1048576" crc="7034f26b" sha1="7be78f23bec38d05240cdfe1186ec0c8291f5a1c"/>
		<rom name="06.03.04_right.u2" size="1048576" crc="6f5f5ef1" sha1="70a43fba4de47ed8dcf38b25eafd5873f3428e72"/>
		<rom name="07010801_left.u70" size="2097152" crc="8e92af68" sha1="00d2bb655b7964a9652896741210ec534df0b0d2"/>
		<rom name="07010801_right.u83" size="2097152" crc="8c148c11" sha1="5ff3be18455b4f04675fec8d5b9d881295c65e23"/>
		<rom name="09011001_left.u70" size="2097152" crc="229c2e63" sha1="91fd2b1acb69efe073647e93db9f11042add2feb"/>
		<rom name="09011001_right.u83" size="2097152" crc="8a853f80" sha1="9a75498f7b02c81a483b4e1c158f35f0ee4c0112"/>
		<rom name="11011501_left.u70" size="2097152" crc="c5cc3461" sha1="5b43c4cb6110a6ccf67cd0f3789253f6872b20c4"/>
		<rom name="11011501_right.u83" size="2097152" crc="de4c3aed" sha1="21596a2edd20eb7de7a4ec8900a270b09c8f326f"/>
		<rom name="11011901_left.u70" size="2097152" crc="d3dd2210" sha1="3548f8cc39859d3f44a55f6bae48966a2d48e0eb"/>
		<rom name="11011901_right.u83" size="2097152" crc="73dcb11c" sha1="69ae4f32a0c9141b2a82ff3935b0cd20333d2964"/>
		<rom name="13012001_left.u70" size="2097152" crc="38e8f659" sha1="88c6acba99b0aca023c6f4d27c061c231490e9e0"/>
		<rom name="13012001_right.u83" size="2097152" crc="e627dbfa" sha1="4fedbe0975ceb7dc0ebebf18a7708d78984db9b7"/>
		<rom name="14010152_left.u70" size="2097152" crc="2716e1ef" sha1="81fe1ae4f9cd1bcb24795ce85913ee22ed0fabcd"/>
		<rom name="14010152_right.u83" size="2097152" crc="7e3f61f6" sha1="1e27d72c35b0c633187159ef434f22398df28882"/>
		<rom name="14011605_left.u70" size="2097152" crc="cd26d4f0" sha1="40822714abf08aeb08d827dbd8cd099f86803754"/>
		<rom name="14011605_right.u83" size="2097152" crc="2bec5b74" sha1="854733cada75e632f01f7096d4740ed4941a3d5b"/>
		<rom name="14011913_left.u70" size="2097152" crc="9a4cefdf" sha1="6c15bc565ede8af19361d60ee1e6657a8055c92c"/>
		<rom name="14011913_right.u83" size="2097152" crc="01d13b89" sha1="b1013366d0803dfbec5a5f90f6a5cea862de0513"/>
		<rom name="15011025_left.u70" size="2097152" crc="c02e14b0" sha1="6bf98927813519dfe60e582dbe5be3ccd87f7c91"/>
		<rom name="15011025_right.u83" size="2097152" crc="bf21a975" sha1="a251b1a7342387300689cd50fe4ce7975b903ac5"/>
		<rom name="19012801_left.u70" size="2097152" crc="b03bd17c" sha1="f281e80f6dda5b727ed71d2deebe3b0ff548773f"/>
		<rom name="19012801_right.u83" size="2097152" crc="5b20a96c" sha1="5fd916b7cc2cdd51bf7dd212c1114f94dc9c7926"/>
		<rom name="20012305_left.u70" size="2097152" crc="ea8961cc" sha1="0ebc7c3b94a6e01ee984af4711043130d9670bd3"/>
		<rom name="20012305_right.u83" size="2097152" crc="e436c1f5" sha1="62ee529cc971fd76aa2ccc15778e3f0c40e3e47f"/>
		<rom name="20012605_left.u70" size="2097152" crc="87331111" sha1="6cdc2d81f68de23af18a975a6f27ddec246be405"/>
		<rom name="20012605_right.u83" size="2097152" crc="045b82ad" sha1="b8e4f9f826970d83ae5fd2f2898de12ad1bf2d24"/>
		<rom name="21012901_left.u70" size="2097152" crc="0d271470" sha1="5cd4b604bfe2fd7e9a8d08e1c7c97f17ae068479"/>
		<rom name="21012901_right.u83" size="2097152" crc="757618f2" sha1="43f9a3e7d544979f8c6974945914d9e099b02abd"/>
		<rom name="24010467_left.u70" size="2097152" crc="9093d820" sha1="05bb14895e3077d277a1d0822036d08f359c0307"/>
		<rom name="24010467_right.u83" size="2097152" crc="eddeff13" sha1="77ccbcf40aeb7305eb13d6d24efafd09955f1eac"/>
		<rom name="24013001_left.u70" size="2097152" crc="06ae7e07" sha1="39a45575b66906d73b519988d1001c99b05c5f34"/>
		<rom name="24013001_right.u83" size="2097152" crc="e97afedf" sha1="10ca3b015afaff5d7812f0f5207b2535602136a5"/>
		<rom name="25012805_left.u70" size="2097152" crc="996f32ce" sha1="cf21bef745986fcbd298167453c7b8e5945ce602"/>
		<rom name="25012805_right.u83" size="2097152" crc="2ecd8da8" sha1="389e9668b2ba4fffed5d2721b2ce70d502fb9f67"/>
		<device_ref name="sh4le"/>
		<device_ref name="ns16550"/>
		<device_ref name="ns16550"/>
		<device_ref name="93c56_16"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
	</machine>
	<machine name="aristmk7" sourcefile="aristocrat/aristmk7.cpp" isbios="yes" runnable="no">
		<description>Aristocrat MK-7 BIOS</description>
		<year>2006?</year>
		<manufacturer>Aristocrat</manufacturer>
		<rom name="mk7-bios_590176_01_1.00.7.u1" size="1048576" crc="f2fea07e" sha1="285038473fbe3a5708045e2f8b14562f3c24b203"/>
		<device_ref name="pentium3"/>
		<device_ref name="pci_root"/>
	</machine>
	<machine name="atarisy1" sourcefile="atari/atarisy1.cpp" isbios="yes" runnable="no">
		<description>Atari System 1 BIOS</description>
		<year>1984</year>
		<manufacturer>Atari Games</manufacturer>
		<biosset name="ttl" description="TTL Motherboard (Rev 2)"/>
		<biosset name="ttl1" description="TTL Motherboard (Rev 1)"/>
		<biosset name="lsi" description="LSI Motherboard"/>
		<rom name="136032.101.e3" size="256" crc="7e84972a" sha1="84d422b53547271e3a07342704a05ef481db3f99"/>
		<rom name="136032.102.e5" size="256" crc="ebf1e0ae" sha1="2d327e78832edd67ca3909c25b8c8c839637a1ed"/>
		<rom name="136032.103.f7" size="235" crc="92d6a0b4" sha1="0a42a4816c89447b16e1f3245409591efea98a4a"/>
		<rom name="136032.104.f5" size="8192" crc="7a29dc07" sha1="72ba464da01bd6d3a91b8d9997d5ac14b6f47aad"/>
		<rom name="136032.105.l13" size="16384" crc="79021d3c" sha1="85febd34bcb166fc3326b5e5e4e80e157b660a08"/>
		<rom name="136032.106.l12" size="16384" crc="76ee86c4" sha1="cbcd424510435a04e9041967a13781fd19b0f2c4"/>
		<rom name="136032.107.b2" size="8192" crc="7a29dc07" sha1="72ba464da01bd6d3a91b8d9997d5ac14b6f47aad"/>
		<rom name="136032.114.j11" size="16384" crc="195c54ad" sha1="d7cda3cd3db4c6f77074ca05e96ae11b62e048b7"/>
		<rom name="136032.115.j10" size="16384" crc="7275b4dc" sha1="0896ab37ea832a1335046353612c1b4c86d8d040"/>
		<rom name="136032.205.l13" size="16384" crc="88d0be26" sha1="d124045eccc562ff0423b23a240e27ad740fa0c9"/>
		<rom name="136032.206.l12" size="16384" crc="3c79ef05" sha1="20fdca7131478e1ee12691bdafd2d5bb74cbd16f"/>
		<device_ref name="m68010"/>
		<device_ref name="m6502"/>
		<device_ref name="2804"/>
		<device_ref name="ls259"/>
		<device_ref name="watchdog"/>
		<device_ref name="timer"/>
		<device_ref name="timer"/>
		<device_ref name="timer"/>
		<device_ref name="gfxdecode"/>
		<device_ref name="palette"/>
		<device_ref name="tilemap"/>
		<device_ref name="tilemap"/>
		<device_ref name="atarimo"/>
		<device_ref name="screen"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="generic_latch_8"/>
		<device_ref name="generic_latch_8"/>
		<device_ref name="ym2151"/>
		<device_ref name="pokey"/>
		<device_ref name="adc0809"/>
		<device_ref name="ipt_merge_all_hi"/>
		<device_ref name="slapstic"/>
	</machine>
	<machine name="awbios" sourcefile="sega/dc_atomiswave.cpp" isbios="yes" runnable="no">
		<description>Atomiswave BIOS</description>
		<year>2001</year>
		<manufacturer>Sammy</manufacturer>
		<biosset name="bios0" description="Sammy BIOS"/>
		<biosset name="bios1" description="Sega BIOS"/>
		<rom name="bios0.ic23" size="131072" crc="719b2b0b" sha1="b4c1a26bc8906d5275eb28c701dff2b9365bcdfa"/>
		<rom name="bios1.ic23" size="131072" crc="d3e80a9f" sha1="33024f9d51c04884c2b44ce146f340e7a857b959"/>
		<rom name="fpr-24363.ic48" size="524288" crc="82a105f0" sha1="5128fe2ddcced77332bdcab691c09958051fa564"/>
		<device_ref name="sh4le"/>
		<device_ref name="timer"/>
		<device_ref name="dc_g2if"/>
		<device_ref name="arm7_le"/>
		<device_ref name="maple_dc"/>
		<device_ref name="screen"/>
		<device_ref name="powervr2"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="aica"/>
		<device_ref name="aicartc"/>
		<device_ref name="macronix_29l001mc"/>
		<device_ref name="aw_rom_board"/>
		<device_ref name="nvram"/>
		<device_ref name="dcctrl"/>
		<device_ref name="dcctrl"/>
	</machine>
	<machine name="bubsys" sourcefile="konami/nemesis.cpp" isbios="yes" runnable="no">
		<description>Bubble System BIOS</description>
		<year>1985</year>
		<manufacturer>Konami</manufacturer>
		<rom name="400a1.2b" size="256" crc="5827b1e8" sha1="fa8cf5f868cfb08bce203baaebb6c4055ee2a000"/>
		<rom name="400a2.1b" size="256" crc="2f44f970" sha1="7ab46f9d5d587665782cefc623b8de0124a6d38a"/>
		<rom name="400b03.8g" size="8192" crc="85c2afc5" sha1="387842d02d50d0d78a27270e7267af19555b9e63"/>
		<rom name="boot.bin" size="480" crc="f0774fc2" sha1="84fade54e025f170d983200a86c1ed96ef1a9ed3"/>
		<rom name="mcu" size="4096" status="nodump"/>
		<device_ref name="m68000"/>
		<device_ref name="timer"/>
		<device_ref name="z80"/>
		<device_ref name="ls259"/>
		<device_ref name="ls259"/>
		<device_ref name="watchdog"/>
		<device_ref name="screen"/>
		<device_ref name="gfxdecode"/>
		<device_ref name="palette"/>
		<device_ref name="speaker"/>
		<device_ref name="generic_latch_8"/>
		<device_ref name="ay8910"/>
		<device_ref name="ay8910"/>
		<device_ref name="filter_rc"/>
		<device_ref name="filter_rc"/>
		<device_ref name="filter_rc"/>
		<device_ref name="filter_rc"/>
		<device_ref name="k005289"/>
		<device_ref name="vlm5030"/>
	</machine>
	<machine name="cdibios" sourcefile="philips/cdi.cpp" isbios="yes" runnable="no">
		<description>CD-i (Mono-I) (PAL) BIOS</description>
		<year>1995</year>
		<manufacturer>Philips</manufacturer>
		<biosset name="mcdi200" description="Magnavox CD-i 200"/>
		<biosset name="pcdi220" description="Philips CD-i 220 F2"/>
		<rom name="cdi200.rom" size="524288" crc="40c4e6b9" sha1="d961de803c89b3d1902d656ceb9ce7c02dccb40a"/>
		<rom name="cdi220b.rom" size="524288" crc="279683ca" sha1="53360a1f21ddac952e95306ced64186a3fc0b93e"/>
		<rom name="zx405042p__cdi_slave_2.0__b43t__zzmk9213.mc68hc705c8a_withtestrom.7206" size="8192" crc="688cda63" sha1="56d0acd7caad51c7de703247cd6d842b36173079" status="baddump"/>
		<device_ref name="scc68070"/>
		<device_ref name="mcd212"/>
		<device_ref name="screen"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
		<device_ref name="cdicdic"/>
		<device_ref name="cdislavehle"/>
		<device_ref name="cdrom_image"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="dmadac"/>
		<device_ref name="dmadac"/>
		<device_ref name="mk48t08"/>
		<device_ref name="software_list"/>
	</machine>
	<machine name="cedmag" sourcefile="efo/cedar_magnet.cpp" isbios="yes" runnable="no">
		<description>Magnet System</description>
		<year>1987</year>
		<manufacturer>EFO SA / Cedar</manufacturer>
		<rom name="magnet-master-vid-e03.bin" size="8192" crc="86c4a4f0" sha1="6db1a006b2e0b2a7cc9748ade881debb098b6757"/>
		<device_ref name="z80"/>
		<device_ref name="address_map_bank"/>
		<device_ref name="address_map_bank"/>
		<device_ref name="address_map_bank"/>
		<device_ref name="z80pio"/>
		<device_ref name="z80pio"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
		<device_ref name="gedmag_sound"/>
		<device_ref name="z80"/>
		<device_ref name="z80ctc"/>
		<device_ref name="z80ctc_channel"/>
		<device_ref name="z80ctc_channel"/>
		<device_ref name="z80ctc_channel"/>
		<device_ref name="z80ctc_channel"/>
		<device_ref name="z80ctc"/>
		<device_ref name="z80ctc_channel"/>
		<device_ref name="z80ctc_channel"/>
		<device_ref name="z80ctc_channel"/>
		<device_ref name="z80ctc_channel"/>
		<device_ref name="generic_latch_8"/>
		<device_ref name="ipt_merge_any_hi"/>
		<device_ref name="speaker"/>
		<device_ref name="ay8910"/>
		<device_ref name="ay8910"/>
		<device_ref name="cd40105"/>
		<device_ref name="msm5205"/>
		<device_ref name="cedmag_plane"/>
		<device_ref name="z80"/>
		<device_ref name="z80pio"/>
		<device_ref name="z80pio"/>
		<device_ref name="cedmag_plane"/>
		<device_ref name="z80"/>
		<device_ref name="z80pio"/>
		<device_ref name="z80pio"/>
		<device_ref name="cedmag_sprite"/>
		<device_ref name="z80"/>
		<device_ref name="z80pio"/>
		<device_ref name="z80pio"/>
		<device_ref name="z80pio"/>
		<device_ref name="address_map_bank"/>
		<device_ref name="cedmag_flop"/>
		<device_ref name="nvram"/>
	</machine>
	<machine name="chihiro" sourcefile="sega/chihiro.cpp" isbios="yes" runnable="no">
		<description>Chihiro BIOS</description>
		<year>2002</year>
		<manufacturer>Sega</manufacturer>
		<biosset name="bios0" description="Chihiro BIOS"/>
		<rom name="315-6351a_epc1pc8.ic2" size="130817" crc="488624ea" sha1="1a607337a186415ae90b48934ce2aae81639d4de"/>
		<rom name="chihiro_xbox_bios.bin" size="524288" crc="66232714" sha1="b700b0041af8f84835e45d1d1250247bf7077188"/>
		<rom name="fpr-23887_29lv160te.ic4" size="2097152" crc="13034372" sha1="77197fba2781ed1d81402c48bd743adb26d3161a"/>
		<rom name="fpr21042_m29w160et.bin" size="2097152" crc="a4fcab0b" sha1="a13cf9c5cdfe8605d82150b7573652f419b30197"/>
		<rom name="ic10_g24lc64.bin" size="8192" crc="cfc5e06f" sha1="3ababd4334d8d57abb22dd98bd2d347df39648d9"/>
		<rom name="ic11_24lc024.bin" size="128" crc="8dc8374e" sha1="cc03a0650bfac4bf6cb66e414bbef121cba53efe"/>
		<rom name="pc20_g24lc64.bin" size="8192" crc="7742ab62" sha1="82dad6e2a75bab4a4840dc6939462f1fb9b95101"/>
		<device_ref name="pentium3"/>
		<device_ref name="pci_root"/>
		<device_ref name="nv2a_host"/>
		<device_ref name="nv2a_ram"/>
		<device_ref name="mcpx_isalpc"/>
		<device_ref name="pic8259"/>
		<device_ref name="pic8259"/>
		<device_ref name="am9517a"/>
		<device_ref name="am9517a"/>
		<device_ref name="pit8254"/>
		<device_ref name="pit_counter"/>
		<device_ref name="pit_counter"/>
		<device_ref name="pit_counter"/>
		<device_ref name="ds12885ext"/>
		<device_ref name="superio_device"/>
		<device_ref name="mcpx_smbus"/>
		<device_ref name="pic16lc"/>
		<device_ref name="cx25871"/>
		<device_ref name="eeprom"/>
		<device_ref name="mcpx_ohci"/>
		<device_ref name="usb_connector"/>
		<device_ref name="ohci_hlean2131qc"/>
		<device_ref name="usb_connector"/>
		<device_ref name="ohci_hlean2131sc"/>
		<device_ref name="usb_connector"/>
		<device_ref name="usb_connector"/>
		<device_ref name="mcpx_ohci"/>
		<device_ref name="mcpx_eth"/>
		<device_ref name="mcpx_apu"/>
		<device_ref name="mcpx_ac97_audio"/>
		<device_ref name="mcpx_ac97_modem"/>
		<device_ref name="pci_bridge"/>
		<device_ref name="mcpx_ide"/>
		<device_ref name="idectrl32bm"/>
		<device_ref name="ata_slot"/>
		<device_ref name="ata_slot"/>
		<device_ref name="ide_baseboard"/>
		<device_ref name="idectrl32bm"/>
		<device_ref name="ata_slot"/>
		<device_ref name="ata_slot"/>
		<device_ref name="nv2a_agp"/>
		<device_ref name="nv2a_gpu"/>
		<device_ref name="screen"/>
		<device_ref name="jvs_master"/>
		<device_ref name="jvs13551"/>
		<device_ref name="tmp90ph44"/>
	</machine>
	<machine name="coh1000a" sourcefile="sony/zn.cpp" isbios="yes" runnable="no">
		<description>Acclaim PSX</description>
		<year>1995</year>
		<manufacturer>Acclaim</manufacturer>
		<rom name="78081g503.ic655" size="8192" status="nodump"/>
		<rom name="ac01.ic652" size="8" crc="c425eaf5" sha1="decf77ab50f7f58c641c3214a11647924f3a8998"/>
		<rom name="m534002c-15.ic353" size="524288" crc="8d8d0764" sha1="7ee83d317190bb1cef2f8f01c81eaaae47150ebb"/>
		<device_ref name="cxd8530cq"/>
		<device_ref name="psxirq"/>
		<device_ref name="psxdma"/>
		<device_ref name="psxmdec"/>
		<device_ref name="psxrcnt"/>
		<device_ref name="psxsio0"/>
		<device_ref name="psxsio1"/>
		<device_ref name="ram"/>
		<device_ref name="cat702"/>
		<device_ref name="znmcu"/>
		<device_ref name="cxd8561q"/>
		<device_ref name="screen"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="psxspu"/>
		<device_ref name="at28c16"/>
		<device_ref name="cat702"/>
	</machine>
	<machine name="coh1000c" sourcefile="sony/zn.cpp" isbios="yes" runnable="no">
		<description>ZN1</description>
		<year>1995</year>
		<manufacturer>Capcom</manufacturer>
		<biosset name="j" description="japan"/>
		<biosset name="e" description="english (debug)"/>
		<rom name="78081g503.ic655" size="8192" status="nodump"/>
		<rom name="cp01.ic652" size="8" crc="bb7ba033" sha1="966f3aee5d00e1312c455f855915d621e6cb0672"/>
		<rom name="m534002c-13.ic353" size="524288" crc="50033af6" sha1="486d92ff6c7f1e54f8e0ef41cd9116eca0e10e1a"/>
		<rom name="msm27c402zb.ic353" size="524288" crc="f20f7fe5" sha1="9aac7d3b3d0cc0bbbe4056164b73078dce41d91c"/>
		<device_ref name="cxd8530cq"/>
		<device_ref name="psxirq"/>
		<device_ref name="psxdma"/>
		<device_ref name="psxmdec"/>
		<device_ref name="psxrcnt"/>
		<device_ref name="psxsio0"/>
		<device_ref name="psxsio1"/>
		<device_ref name="ram"/>
		<device_ref name="cat702"/>
		<device_ref name="znmcu"/>
		<device_ref name="cxd8561q"/>
		<device_ref name="screen"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="psxspu"/>
		<device_ref name="at28c16"/>
		<device_ref name="cat702"/>
		<device_ref name="z80"/>
		<device_ref name="generic_latch_8"/>
		<device_ref name="qsound_hle"/>
	</machine>
	<machine name="coh1000t" sourcefile="sony/zn.cpp" isbios="yes" runnable="no">
		<description>Taito FX1</description>
		<year>1995</year>
		<manufacturer>Taito</manufacturer>
		<rom name="78081g503.ic655" size="8192" status="nodump"/>
		<rom name="m534002c-14.ic353" size="524288" crc="e3f23b6e" sha1="e18907cf8c6ba54d96edba0a9a00487a90219e0d"/>
		<rom name="tt01.ic652" size="8" crc="daac13e7" sha1="96d94f2b06fb7ecd91454969f4959a583ffb9d5a"/>
		<device_ref name="cxd8530cq"/>
		<device_ref name="psxirq"/>
		<device_ref name="psxdma"/>
		<device_ref name="psxmdec"/>
		<device_ref name="psxrcnt"/>
		<device_ref name="psxsio0"/>
		<device_ref name="psxsio1"/>
		<device_ref name="ram"/>
		<device_ref name="cat702"/>
		<device_ref name="znmcu"/>
		<device_ref name="cxd8561q"/>
		<device_ref name="screen"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="psxspu"/>
		<device_ref name="at28c16"/>
		<device_ref name="cat702"/>
		<device_ref name="z80"/>
		<device_ref name="ym2610b"/>
		<device_ref name="mb3773"/>
		<device_ref name="tc0140syt"/>
	</machine>
	<machine name="coh1000w" sourcefile="sony/zn.cpp" isbios="yes" runnable="no">
		<description>Atari PSX</description>
		<year>1996</year>
		<manufacturer>Atari</manufacturer>
		<rom name="78081g503.ic655" size="8192" status="nodump"/>
		<rom name="msm27c402zb.ic353" size="524288" crc="45e8a4b4" sha1="815488d8563c85f97fbc3384ff21f08e4c88b7b7"/>
		<rom name="tw01.ic652" size="8" crc="1cac067e" sha1="8e87941bfb374172628c8a37647e3a66b7166aa8"/>
		<device_ref name="cxd8530cq"/>
		<device_ref name="psxirq"/>
		<device_ref name="psxdma"/>
		<device_ref name="psxmdec"/>
		<device_ref name="psxrcnt"/>
		<device_ref name="psxsio0"/>
		<device_ref name="psxsio1"/>
		<device_ref name="ram"/>
		<device_ref name="cat702"/>
		<device_ref name="znmcu"/>
		<device_ref name="cxd8561q"/>
		<device_ref name="screen"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="psxspu"/>
		<device_ref name="at28c16"/>
		<device_ref name="cat702"/>
		<device_ref name="watchdog"/>
		<device_ref name="vt83c461"/>
		<device_ref name="ata_slot"/>
		<device_ref name="idehd"/>
		<device_ref name="harddisk_image"/>
		<device_ref name="ata_slot"/>
	</machine>
	<machine name="coh1001l" sourcefile="sony/zn.cpp" isbios="yes" runnable="no">
		<description>Atlus PSX</description>
		<year>1996</year>
		<manufacturer>Atlus</manufacturer>
		<rom name="78081g503.ic655" size="8192" status="nodump"/>
		<rom name="at01.ic652" size="8" crc="181668b3" sha1="8d2fe1facb4473cc20b4b477aaf881f9280939cf"/>
		<rom name="m534002c-17.ic353" size="524288" crc="6721146b" sha1="9511d24bfe25eb180fb2db0835b131cb4a12730e"/>
		<device_ref name="cxd8530cq"/>
		<device_ref name="psxirq"/>
		<device_ref name="psxdma"/>
		<device_ref name="psxmdec"/>
		<device_ref name="psxrcnt"/>
		<device_ref name="psxsio0"/>
		<device_ref name="psxsio1"/>
		<device_ref name="ram"/>
		<device_ref name="cat702"/>
		<device_ref name="znmcu"/>
		<device_ref name="cxd8561q"/>
		<device_ref name="screen"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="psxspu"/>
		<device_ref name="at28c16"/>
		<device_ref name="cat702"/>
		<device_ref name="m68000"/>
		<device_ref name="generic_latch_16"/>
		<device_ref name="ymz280b"/>
	</machine>
	<machine name="coh1002e" sourcefile="sony/zn.cpp" isbios="yes" runnable="no">
		<description>PS Arcade 95</description>
		<year>1997</year>
		<manufacturer>Eighting / Raizing</manufacturer>
		<rom name="78081g503.ic655" size="8192" status="nodump"/>
		<rom name="et01.ic652" size="8" crc="a7dd922e" sha1="1069c1d9015028a51a1b314cfacb014ea90aa425"/>
		<rom name="m27c402cz-54.ic353" size="524288" crc="910f3a8b" sha1="cd68532967a25f476a6d73473ec6b6f4df2e1689"/>
		<device_ref name="cxd8530cq"/>
		<device_ref name="psxirq"/>
		<device_ref name="psxdma"/>
		<device_ref name="psxmdec"/>
		<device_ref name="psxrcnt"/>
		<device_ref name="psxsio0"/>
		<device_ref name="psxsio1"/>
		<device_ref name="ram"/>
		<device_ref name="cat702"/>
		<device_ref name="znmcu"/>
		<device_ref name="cxd8561q"/>
		<device_ref name="screen"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="psxspu"/>
		<device_ref name="at28c16"/>
		<device_ref name="cat702"/>
		<device_ref name="m68000"/>
		<device_ref name="generic_latch_8"/>
		<device_ref name="ymf271"/>
	</machine>
	<machine name="coh1002m" sourcefile="sony/zn.cpp" isbios="yes" runnable="no">
		<description>TPS</description>
		<year>1997</year>
		<manufacturer>Tecmo</manufacturer>
		<rom name="78081g503.ic655" size="8192" status="nodump"/>
		<rom name="m534002c-61.ic353" size="524288" crc="69ffbcb4" sha1="03eb2febfab3fcde716defff291babd9392de965"/>
		<rom name="mg01.ic652" size="8" crc="50dc8322" sha1="cef4011c6c06d6fce546e1db5d9fbae155eabf57"/>
		<device_ref name="cxd8530cq"/>
		<device_ref name="psxirq"/>
		<device_ref name="psxdma"/>
		<device_ref name="psxmdec"/>
		<device_ref name="psxrcnt"/>
		<device_ref name="psxsio0"/>
		<device_ref name="psxsio1"/>
		<device_ref name="ram"/>
		<device_ref name="cat702"/>
		<device_ref name="znmcu"/>
		<device_ref name="cxd8561q"/>
		<device_ref name="screen"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="psxspu"/>
		<device_ref name="at28c16"/>
		<device_ref name="cat702"/>
	</machine>
	<machine name="coh1002v" sourcefile="sony/zn.cpp" isbios="yes" runnable="no">
		<description>Video System PSX</description>
		<year>1996</year>
		<manufacturer>Video System Co.</manufacturer>
		<rom name="78081g503.ic655" size="8192" status="nodump"/>
		<rom name="coh-1002v.ic353" size="524288" crc="5ff165f3" sha1="8f59314c1093446b9bcb06d232244da6df78e206"/>
		<rom name="kn01.ic652" size="8" crc="1ce271df" sha1="b01479dc75a4a8a86bee7ac7cd10af2bda332544"/>
		<device_ref name="cxd8530cq"/>
		<device_ref name="psxirq"/>
		<device_ref name="psxdma"/>
		<device_ref name="psxmdec"/>
		<device_ref name="psxrcnt"/>
		<device_ref name="psxsio0"/>
		<device_ref name="psxsio1"/>
		<device_ref name="ram"/>
		<device_ref name="cat702"/>
		<device_ref name="znmcu"/>
		<device_ref name="cxd8561q"/>
		<device_ref name="screen"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="psxspu"/>
		<device_ref name="at28c16"/>
		<device_ref name="cat702"/>
	</machine>
	<machine name="coh3002c" sourcefile="sony/zn.cpp" isbios="yes" runnable="no">
		<description>ZN2</description>
		<year>1997</year>
		<manufacturer>Capcom</manufacturer>
		<rom name="78081g503.ic655" size="8192" status="nodump"/>
		<rom name="cp10.ic652" size="8" crc="7808fcef" sha1="3c3fb8227b05dace042dc1429b9f2355b1a15638"/>
		<rom name="m534002c-59.ic353" size="524288" crc="e860ea8b" sha1="66e7e1d4e426466b8f48a2ba055a91b475569504"/>
		<device_ref name="cxd8661r"/>
		<device_ref name="psxirq"/>
		<device_ref name="psxdma"/>
		<device_ref name="psxmdec"/>
		<device_ref name="psxrcnt"/>
		<device_ref name="psxsio0"/>
		<device_ref name="psxsio1"/>
		<device_ref name="ram"/>
		<device_ref name="cat702"/>
		<device_ref name="znmcu"/>
		<device_ref name="cxd8654q"/>
		<device_ref name="screen"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="psxspu"/>
		<device_ref name="at28c16"/>
		<device_ref name="cat702"/>
		<device_ref name="z80"/>
		<device_ref name="generic_latch_8"/>
		<device_ref name="qsound_hle"/>
	</machine>
	<machine name="coh3002t" sourcefile="sony/taitogn.cpp" isbios="yes" runnable="no">
		<description>Taito GNET</description>
		<year>1997</year>
		<manufacturer>Taito</manufacturer>
		<biosset name="v1" description="G-NET BIOS v1 flasher"/>
		<biosset name="v2" description="G-NET BIOS v2 flasher"/>
		<rom name="f35-01_m27c800.bin" size="1048576" crc="6225ec11" sha1="047852d456b6ff85f8e640887caa03cf3e63ffad"/>
		<rom name="f35-01_m27c800_v1.bin" size="1048576" crc="cd15cc30" sha1="78361f46fa7186d5058937c86c66247a86b1257f"/>
		<rom name="flash.u30" size="2097152" crc="c48c8236" sha1="c6dad60266ce2ff635696bc0d91903c543273559"/>
		<rom name="m534002c-60.ic353" size="524288" crc="03967fa7" sha1="0e17fec2286e4e25deb23d40e41ce0986f373d49"/>
		<rom name="tt10.ic652" size="8" crc="235510b1" sha1="2cc02113207a8f0b078152d31ce6503411750e70"/>
		<rom name="tt16" size="8" crc="6bb167b3" sha1="9dcba08f10775a9adf2b1f382c947460edd3d239"/>
		<rom name="upd78081.655" size="8192" status="nodump"/>
		<device_ref name="cxd8661r"/>
		<device_ref name="psxirq"/>
		<device_ref name="psxdma"/>
		<device_ref name="psxmdec"/>
		<device_ref name="psxrcnt"/>
		<device_ref name="psxsio0"/>
		<device_ref name="psxsio1"/>
		<device_ref name="ram"/>
		<device_ref name="cat702"/>
		<device_ref name="znmcu"/>
		<device_ref name="cxd8654q"/>
		<device_ref name="screen"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="psxspu"/>
		<device_ref name="at28c16"/>
		<device_ref name="cat702"/>
		<device_ref name="rf5c296"/>
		<device_ref name="pccard"/>
		<device_ref name="mb3773"/>
		<device_ref name="intel_te28f160"/>
		<device_ref name="intel_e28f400b"/>
		<device_ref name="intel_te28f160"/>
		<device_ref name="intel_te28f160"/>
		<device_ref name="intel_te28f160"/>
		<device_ref name="address_map_bank"/>
		<device_ref name="taito_zoom"/>
		<device_ref name="mn1020012a"/>
		<device_ref name="tms57002"/>
		<device_ref name="zsg2"/>
	</machine>
	<machine name="crysbios" sourcefile="misc/crystal.cpp" isbios="yes" runnable="no">
		<description>Crystal System BIOS</description>
		<year>2001</year>
		<manufacturer>BrezzaSoft</manufacturer>
		<biosset name="amg0110b" description="AMG0110B PCB"/>
		<biosset name="amg0110d" description="AMG0110D PCB"/>
		<rom name="mx27l1000-alt.u14" size="131072" crc="1e8175c8" sha1="f60c016be2ff11e47b2192acddb92676043af501"/>
		<rom name="mx27l1000.u14" size="131072" crc="beff39a9" sha1="b6f6dda58d9c82273f9422c1bd623411e58982cb"/>
		<device_ref name="se3208"/>
		<device_ref name="nvram"/>
		<device_ref name="vrender0"/>
		<device_ref name="vr0uart"/>
		<device_ref name="vr0uart"/>
		<device_ref name="screen"/>
		<device_ref name="vr0video"/>
		<device_ref name="palette"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="vr0sound"/>
		<device_ref name="ds1302"/>
	</machine>
	<machine name="cubo" sourcefile="amiga/cubo.cpp" isbios="yes" runnable="no">
		<description>Cubo BIOS</description>
		<year>1993</year>
		<manufacturer>Commodore</manufacturer>
		<biosset name="cd32" description="Kickstart v3.1 rev 40.60 with CD32 Extended-ROM"/>
		<rom name="391640-03.u6a" size="1048576" crc="d3837ae4" sha1="06807db3181637455f4d46582d9972afec8956d9"/>
		<device_ref name="m68ec020"/>
		<device_ref name="address_map_bank"/>
		<device_ref name="address_map_bank"/>
		<device_ref name="agnus_copper"/>
		<device_ref name="24c08"/>
		<device_ref name="akiko"/>
		<device_ref name="cdrom_image"/>
		<device_ref name="cdda"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="paula_8364"/>
		<device_ref name="mos8520"/>
		<device_ref name="mos8520"/>
		<device_ref name="microtouch"/>
		<device_ref name="paula_fdc"/>
	</machine>
	<machine name="decocass" sourcefile="dataeast/decocass.cpp" isbios="yes" runnable="no">
		<description>DECO Cassette System</description>
		<year>1981</year>
		<manufacturer>Data East Corporation</manufacturer>
		<biosset name="a" description="BIOS A (Japan)"/>
		<biosset name="b" description="BIOS B (USA)"/>
		<biosset name="c" description="BIOS C (UK)"/>
		<biosset name="d" description="BIOS D (Europe)"/>
		<biosset name="a0" description="BIOS A (Japan, older PCB)"/>
		<biosset name="b0" description="BIOS B (USA, older PCB)"/>
		<biosset name="c0" description="BIOS C (UK, older PCB)"/>
		<biosset name="d0" description="BIOS D (Europe, older PCB)"/>
		<rom name="cassmcu.1c" size="1024" crc="a6df18fd" sha1="1f9ea47e372d31767c936c15852b43df2b0ee8ff"/>
		<rom name="dsp-3_p0-a.m9" size="2048" crc="2541e34b" sha1="4f983513dbae1350c83a433dea77a4465748b9c6"/>
		<rom name="dsp-3_p0-b.m9" size="2048" crc="b67a91d9" sha1="681c040be0f0ed1ba0a50161b36d0ad8e1c8c5cb"/>
		<rom name="dsp-3_p0-c.m9" size="2048" crc="c76c4057" sha1="4093d4ac44feff595e34f361ed1ed84113c9225e"/>
		<rom name="dsp-3_p0-d.m9" size="2048" crc="4b7d72bc" sha1="a70c5ba88404dafee2cc717071c4a249f67ab645"/>
		<rom name="dsp-3_p1-.l9" size="2048" crc="3bfff5f3" sha1="4e9437cb1b76d64da6b37f01bd6e879fb399e8ce"/>
		<rom name="dsp-3_p3-.e5" size="32" crc="539a5a64" sha1="7b7d3cc58ac6f95242240c97046e770d2fd20c96"/>
		<rom name="dsp-3_p5-.m4" size="32" crc="e52089a0" sha1="d85c17809b089c6977ee9571f976af6f107fd4d3"/>
		<rom name="rms-3_p2-.c9" size="1024" crc="6c4a891f" sha1="5c00cf8b1accfdbb1d61e9b3f6db1594dfbc608b"/>
		<rom name="rms-3_p4-.f6" size="32" crc="9014c0fd" sha1="7405d39a5f4fcad821448ddaf6bd4e27c0c9e145"/>
		<rom name="v0a-.7e" size="4096" crc="3d33ac34" sha1="909d59e7a993affd10224402b4370e82a5f5545c"/>
		<rom name="v0b-.7e" size="4096" crc="23d929b7" sha1="063f83020ba3d6f43ab8471f95ca919767b93aa4"/>
		<rom name="v0c-.7e" size="4096" crc="9f505709" sha1="a9c661ba5a0d3fa5e935fb9c10fa63e2d9809981"/>
		<rom name="v0d-.7e" size="4096" crc="1e0c22b1" sha1="5fec8fef500bbebc13d0173406afc55235d3affb"/>
		<rom name="v1-.5a" size="2048" crc="b66b2c2a" sha1="0097f38beb4872e735e560148052e258a26b08fd"/>
		<rom name="v2.3m" size="32" crc="238fdb40" sha1="b88e8fabb82092105c3828154608ea067acbf2e5"/>
		<rom name="v3.3j" size="32" crc="51eef657" sha1="eaedce5caf55624ad6ae706aedf82c5717c60f1f"/>
		<rom name="v4.10d" size="32" crc="3b5836b4" sha1="b630bb277d9ec09d46ef26b944014dd6165b35d8"/>
		<device_ref name="deco222"/>
		<device_ref name="m6502"/>
		<device_ref name="timer"/>
		<device_ref name="i8041a"/>
		<device_ref name="watchdog"/>
		<device_ref name="decocass_tape"/>
		<device_ref name="screen"/>
		<device_ref name="gfxdecode"/>
		<device_ref name="palette"/>
		<device_ref name="speaker"/>
		<device_ref name="generic_latch_8"/>
		<device_ref name="generic_latch_8"/>
		<device_ref name="ay8910"/>
		<device_ref name="ay8910"/>
	</machine>
	<machine name="f355bios" sourcefile="sega/naomi.cpp" isbios="yes" runnable="no">
		<description>NAOMI Ferrari F355 Challenge (twin-deluxe) BIOS</description>
		<year>1999</year>
		<manufacturer>Sega</manufacturer>
		<biosset name="bios0" description="Ferrari F355 (Export)"/>
		<biosset name="bios1" description="Ferrari F355 (USA)"/>
		<biosset name="bios2" description="Ferrari F355 (Japan)"/>
		<rom name="epr-22849.ic27" size="2097152" crc="121e009c" sha1="3beb91f660e60590491b209b6be8584b05a90548"/>
		<rom name="epr-22850.ic27" size="2097152" crc="28aa539d" sha1="14485368656af80504b212da620179c49f84c1a2"/>
		<rom name="epr-22851.ic27" size="2097152" crc="62483677" sha1="3e3bcacf5f972c376b569f45307ee7fd0b5031b7"/>
		<rom name="main_eeprom.bin" size="128" crc="fea29cbb" sha1="4099f1747aafa07db34f6e072cd9bfaa83bae10e"/>
		<rom name="x76f100_eeprom.bin" size="132" crc="3ea24b6a" sha1="3a730ebcf56e0060fef6b1b02eb2eb7cfb7e61dc"/>
		<device_ref name="sh4le"/>
		<device_ref name="timer"/>
		<device_ref name="dc_g2if"/>
		<device_ref name="arm7_le"/>
		<device_ref name="maple_dc"/>
		<device_ref name="screen"/>
		<device_ref name="powervr2"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="aica"/>
		<device_ref name="aicartc"/>
		<device_ref name="93c46_16"/>
		<device_ref name="mie"/>
		<device_ref name="z80"/>
		<device_ref name="mie_jvs"/>
		<device_ref name="jvs13551"/>
		<device_ref name="tmp90ph44"/>
		<device_ref name="93c46_8"/>
		<device_ref name="x76f100"/>
		<device_ref name="m3comm"/>
		<device_ref name="m68000"/>
		<device_ref name="ram"/>
		<device_ref name="nvram"/>
		<device_ref name="naomi_rom_board"/>
	</machine>
	<machine name="f355dlx" sourcefile="sega/naomi.cpp" isbios="yes" runnable="no">
		<description>NAOMI Ferrari F355 Challenge (deluxe) BIOS</description>
		<year>1999</year>
		<manufacturer>Sega</manufacturer>
		<biosset name="bios0" description="Ferrari F355 Deluxe (Export)"/>
		<biosset name="bios1" description="Ferrari F355 Deluxe (USA)"/>
		<biosset name="bios2" description="Ferrari F355 Deluxe (Japan)"/>
		<biosset name="bios3" description="Ferrari F355 Deluxe (Export, prototype)"/>
		<biosset name="bios4" description="Ferrari F355 Deluxe (Japan, prototype)"/>
		<rom name="epr-21862.ic27" size="2097152" crc="1f630716" sha1="8d157809770467c3e7618c6299f3b96b5f10518c"/>
		<rom name="epr-21862p.ic27" size="2097152" crc="f0cd4aaa" sha1="9a9157992bf7a104c096efcdb8b02ceece186cbb"/>
		<rom name="epr-21863.ic27" size="2097152" crc="0615a4d1" sha1="2c6986580b84278af75f396229fdd587bebc1768"/>
		<rom name="epr-21864.ic27" size="2097152" crc="12ed7c66" sha1="046be66e92eae766f3e05594aa837fc8888534ed"/>
		<rom name="epr-21864p.ic27" size="2097152" crc="05128861" sha1="5bdb320d84015b8429527a8eb4524958031862aa"/>
		<rom name="main_eeprom.bin" size="128" crc="fea29cbb" sha1="4099f1747aafa07db34f6e072cd9bfaa83bae10e"/>
		<rom name="x76f100_eeprom.bin" size="132" crc="3ea24b6a" sha1="3a730ebcf56e0060fef6b1b02eb2eb7cfb7e61dc"/>
		<device_ref name="sh4le"/>
		<device_ref name="timer"/>
		<device_ref name="dc_g2if"/>
		<device_ref name="arm7_le"/>
		<device_ref name="maple_dc"/>
		<device_ref name="screen"/>
		<device_ref name="powervr2"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="aica"/>
		<device_ref name="aicartc"/>
		<device_ref name="93c46_16"/>
		<device_ref name="mie"/>
		<device_ref name="z80"/>
		<device_ref name="mie_jvs"/>
		<device_ref name="jvs13551"/>
		<device_ref name="tmp90ph44"/>
		<device_ref name="93c46_8"/>
		<device_ref name="x76f100"/>
		<device_ref name="m3comm"/>
		<device_ref name="m68000"/>
		<device_ref name="ram"/>
		<device_ref name="nvram"/>
		<device_ref name="naomi_rom_board"/>
	</machine>
	<machine name="galgbios" sourcefile="ces/galgames.cpp" isbios="yes" runnable="no">
		<description>Galaxy Games BIOS</description>
		<year>1998</year>
		<manufacturer>Creative Electronics &amp; Software</manufacturer>
		<biosset name="1.90" description="v1.90 12/01/98"/>
		<biosset name="1.80" description="v1.80 10/05/98"/>
		<rom name="16v8h-blue.u24" size="279" status="nodump"/>
		<rom name="16v8h-green.u27" size="279" status="nodump"/>
		<rom name="16v8h-magenta.u26" size="279" status="nodump"/>
		<rom name="16v8h-red.u45" size="279" status="nodump"/>
		<rom name="16v8h-yellow.u25" size="279" status="nodump"/>
		<rom name="galaxy_u1__v1.80_10-15-98.u1" size="1048576" crc="e3ae423c" sha1="66d1964845a99a5ed4b19b4135b55cde6b5fe295"/>
		<rom name="galaxy_u1__v1.90_12-01-98.u1" size="1048576" crc="c6d7bc6d" sha1="93c032f9aa38cbbdda59a8a25ff9f38f7ad9c760"/>
		<rom name="galaxy_u2__v1.80_10-15-98.u2" size="1048576" crc="73cff284" sha1="e6f7d92999cdb478c21c3b65a04eade84299ac12"/>
		<rom name="galaxy_u2__v1.90_12-01-98.u2" size="1048576" crc="e51ff184" sha1="aaa795f2c15ec29b3ceeb5c917b643db0dbb7083"/>
		<device_ref name="m68000"/>
		<device_ref name="timer"/>
		<device_ref name="watchdog"/>
		<device_ref name="starpak_slot"/>
		<device_ref name="galgames_bios_cart"/>
		<device_ref name="93c76_8"/>
		<device_ref name="screen"/>
		<device_ref name="cesblit"/>
		<device_ref name="palette"/>
		<device_ref name="speaker"/>
		<device_ref name="okim6295"/>
		<device_ref name="starpak_cart"/>
		<device_ref name="starpak_cart"/>
		<device_ref name="starpak_cart"/>
		<device_ref name="starpak_cart"/>
	</machine>
	<machine name="genpin">
		<description>genpin</description>
		<sample name="bumper"/>
		<sample name="chime1"/>
		<sample name="chime2"/>
		<sample name="chime3"/>
		<sample name="chime4"/>
		<sample name="coil_coinlockout_engage"/>
		<sample name="coil_coinlockout_release"/>
		<sample name="coinin"/>
		<sample name="drop_target_reset"/>
		<sample name="hole"/>
		<sample name="kickback"/>
		<sample name="knocker"/>
		<sample name="outhole"/>
		<sample name="relay_engage"/>
		<sample name="relay_release"/>
		<sample name="sling"/>
		<sample name="solenoid_engage"/>
		<sample name="solenoid_release"/>
	</machine>
	<machine name="gp_110" sourcefile="pinball/gp_1.cpp" sampleof="genpin" isbios="yes" runnable="no">
		<description>Model 110</description>
		<year>1978</year>
		<manufacturer>Game Plan</manufacturer>
		<rom name="a-110.u12" size="2048" crc="ed0d518b" sha1="8f3ca8792ad907c660d9149a1aa3a3528c7573e3"/>
		<rom name="b1-110.u13" size="2048" crc="a223f2e8" sha1="767e15e19e11399935c890c1d1034dccf1ad7f92"/>
		<device_ref name="z80"/>
		<device_ref name="nvram"/>
		<device_ref name="speaker"/>
		<device_ref name="samples"/>
		<device_ref name="i8255"/>
		<device_ref name="z80ctc"/>
		<device_ref name="z80ctc_channel"/>
		<device_ref name="z80ctc_channel"/>
		<device_ref name="z80ctc_channel"/>
		<device_ref name="z80ctc_channel"/>
		<device_ref name="clock"/>
		<sample name="bumper"/>
		<sample name="chime1"/>
		<sample name="chime2"/>
		<sample name="chime3"/>
		<sample name="chime4"/>
		<sample name="coil_coinlockout_engage"/>
		<sample name="coil_coinlockout_release"/>
		<sample name="coinin"/>
		<sample name="drop_target_reset"/>
		<sample name="hole"/>
		<sample name="kickback"/>
		<sample name="knocker"/>
		<sample name="outhole"/>
		<sample name="relay_engage"/>
		<sample name="relay_release"/>
		<sample name="sling"/>
		<sample name="solenoid_engage"/>
		<sample name="solenoid_release"/>
	</machine>
	<machine name="gq863" sourcefile="konami/twinkle.cpp" isbios="yes" runnable="no">
		<description>Twinkle System</description>
		<year>1999</year>
		<manufacturer>Konami</manufacturer>
		<rom name="863a03.7b" size="524288" crc="81498f73" sha1="3599b40a5872eab3a00d345287635355fcb25a71"/>
		<rom name="863a05.2x" size="524288" crc="6f42a09e" sha1="cab5209f90f47b9ee6e721479913ad74e3ba84b1"/>
		<device_ref name="cxd8530cq"/>
		<device_ref name="psxirq"/>
		<device_ref name="psxdma"/>
		<device_ref name="psxmdec"/>
		<device_ref name="psxrcnt"/>
		<device_ref name="psxsio0"/>
		<device_ref name="psxsio1"/>
		<device_ref name="ram"/>
		<device_ref name="m68000"/>
		<device_ref name="watchdog"/>
		<device_ref name="cy7c131"/>
		<device_ref name="nscsi_bus"/>
		<device_ref name="nscsi_connector"/>
		<device_ref name="nxm5401"/>
		<device_ref name="cdrom_image"/>
		<device_ref name="cdda"/>
		<device_ref name="nscsi_connector"/>
		<device_ref name="ncr53cf96"/>
		<device_ref name="ata_interface"/>
		<device_ref name="ata_slot"/>
		<device_ref name="idehd"/>
		<device_ref name="harddisk_image"/>
		<device_ref name="ata_slot"/>
		<device_ref name="rtc65271"/>
		<device_ref name="fdc37c665gt"/>
		<device_ref name="n82077aa"/>
		<device_ref name="pc_lpt"/>
		<device_ref name="centronics"/>
		<device_ref name="centronics_printer"/>
		<device_ref name="printer_image"/>
		<device_ref name="input_buffer"/>
		<device_ref name="input_buffer"/>
		<device_ref name="input_buffer"/>
		<device_ref name="output_latch"/>
		<device_ref name="output_latch"/>
		<device_ref name="ns16550"/>
		<device_ref name="ns16550"/>
		<device_ref name="cxd8561q"/>
		<device_ref name="screen"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="psxspu"/>
		<device_ref name="rf5c400"/>
	</machine>
	<machine name="gts1" sourcefile="pinball/gts1.cpp" sampleof="genpin" isbios="yes" runnable="no">
		<description>System 1</description>
		<year>1977</year>
		<manufacturer>Gottlieb</manufacturer>
		<rom name="a1752cf.u5" size="2048" crc="614a3bd9" sha1="febca18fb6f96037ca82e515dd161dfcb0e4c776"/>
		<rom name="a1753ce.u4" size="2048" crc="4cd312dd" sha1="31245daa9972ef8652caee69986585bb8239e86e"/>
		<device_ref name="pps4_2"/>
		<device_ref name="nvram"/>
		<device_ref name="ra17xx"/>
		<device_ref name="ra17xx"/>
		<device_ref name="r10696"/>
		<device_ref name="r10696"/>
		<device_ref name="r10788"/>
		<device_ref name="speaker"/>
		<device_ref name="samples"/>
		<sample name="bumper"/>
		<sample name="chime1"/>
		<sample name="chime2"/>
		<sample name="chime3"/>
		<sample name="chime4"/>
		<sample name="coil_coinlockout_engage"/>
		<sample name="coil_coinlockout_release"/>
		<sample name="coinin"/>
		<sample name="drop_target_reset"/>
		<sample name="hole"/>
		<sample name="kickback"/>
		<sample name="knocker"/>
		<sample name="outhole"/>
		<sample name="relay_engage"/>
		<sample name="relay_release"/>
		<sample name="sling"/>
		<sample name="solenoid_engage"/>
		<sample name="solenoid_release"/>
	</machine>
	<machine name="hikaru" sourcefile="sega/hikaru.cpp" isbios="yes" runnable="no">
		<description>Hikaru BIOS</description>
		<year>2000</year>
		<manufacturer>Sega</manufacturer>
		<biosset name="bios0" description="epr23400a"/>
		<biosset name="bios1" description="epr23400"/>
		<biosset name="bios2" description="epr21904"/>
		<biosset name="bios3" description="Development / prototype"/>
		<rom name="epr-21904.ic94" size="2097152" crc="d96298b6" sha1="d10d837bc7d68eb7125c34beffe21a91305627b0"/>
		<rom name="epr-23400.ic94" size="2097152" crc="3d557104" sha1="d39879f5a1acbd54ad8ee4fbd412f870c9ff4aa5"/>
		<rom name="epr-23400a.ic94" size="2097152" crc="2aa906a7" sha1="098c9909b123ed6c338ac874f2ee90e3b2da4c02"/>
		<rom name="prot_bot.ic94" size="2097152" crc="7cbf2fb6" sha1="7384e3c9314add7d61f93c9edd9fb7788d08f423"/>
		<device_ref name="sh4le"/>
		<device_ref name="sh4le"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
	</machine>
	<machine name="hng64" sourcefile="snk/hng64.cpp" isbios="yes" runnable="no">
		<description>Hyper NeoGeo 64 BIOS</description>
		<year>1997</year>
		<manufacturer>SNK</manufacturer>
		<biosset name="japan" description="Japan"/>
		<biosset name="us" description="USA"/>
		<biosset name="export" description="Export" default="yes"/>
		<biosset name="korea" description="Korea"/>
		<rom name="bios_export.bin" size="524288" crc="bbf07ec6" sha1="5656aa077f6a6d43953f15b5123eea102a9d5313"/>
		<rom name="bios_korea.bin" size="524288" crc="ac953e2e" sha1="f502188ef252b7c9d04934c4b525730a116de48b"/>
		<rom name="bios_us.bin" size="524288" crc="ab5948d6" sha1="f8b940c1ae5ce2d3b2cd0c9bfaf6e5b063cec06e"/>
		<rom name="brom1.bin" size="524288" crc="a30dd3de" sha1="3e2fd0a56214e6f5dcb93687e409af13d065ea30"/>
		<rom name="from1.bin" size="524288" crc="6b933005" sha1="e992747f46c48b66e5509fe0adf19c91250b00c7"/>
		<rom name="lvs-igx-br9020f.u3" size="256" crc="af9f4287" sha1="6df0e35c77dbfee2fab7ff490dcd651db420e367"/>
		<rom name="lvs-ioj-br9020f.u2" size="256" crc="78b7020d" sha1="2b8549532ef5e1e8102dbe71af55fdfb27ccbba6"/>
		<rom name="lvs-jam-br9020f.u3" size="256" crc="dabec5d2" sha1="19c5be89c57387d6ea563b3dc55674d0692af98e"/>
		<rom name="rom1.bin" size="130866" crc="4a6832dc" sha1="ae504f7733c2f40450157cd1d3b85bc83fac8569"/>
		<rom name="tmp87ph40an.bin" size="32768" crc="b70df21f" sha1="5b742e8a0bbf4c0ae4f4398d34c7058fb24acc92"/>
		<device_ref name="vr4300be"/>
		<device_ref name="timer"/>
		<device_ref name="nvram"/>
		<device_ref name="rtc62423"/>
		<device_ref name="gfxdecode"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
		<device_ref name="palette"/>
		<device_ref name="palette"/>
		<device_ref name="palette"/>
		<device_ref name="v53a"/>
		<device_ref name="pit8254"/>
		<device_ref name="pit_counter"/>
		<device_ref name="pit_counter"/>
		<device_ref name="pit_counter"/>
		<device_ref name="v5x_dmau"/>
		<device_ref name="v5x_icu"/>
		<device_ref name="v5x_scu"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="l7a1045"/>
		<device_ref name="kl5c80a12"/>
		<device_ref name="kp69"/>
		<device_ref name="kp64"/>
		<device_ref name="kp64"/>
		<device_ref name="kp63_3channel"/>
		<device_ref name="tmp87ph40an"/>
		<device_ref name="idt71321"/>
		<device_ref name="hng64_lamps"/>
	</machine>
	<machine name="hod2bios" sourcefile="sega/naomi.cpp" isbios="yes" runnable="no">
		<description>NAOMI The House of the Dead 2 BIOS</description>
		<year>1998</year>
		<manufacturer>Sega</manufacturer>
		<biosset name="bios0" description="HOTD2 (Export)"/>
		<biosset name="bios1" description="HOTD2 (USA)"/>
		<biosset name="bios2" description="HOTD2 (Japan)"/>
		<biosset name="bios3" description="HOTD2 (Korea)"/>
		<biosset name="bios4" description="HOTD2 (Proto)"/>
		<rom name="epr-21329.ic27" size="2097152" crc="d99e5b9b" sha1="453ffb41b6197cac6d12e7814bb1d7281ccf1659"/>
		<rom name="epr-21330.ic27" size="2097152" crc="9e3bfa1b" sha1="b539d38c767b0551b8e7956c1ff795de8bbe2fbc"/>
		<rom name="epr-21331.ic27" size="2097152" crc="065f8500" sha1="49a3881e8d76f952ef5e887200d77b4a415d47fe"/>
		<rom name="epr-21332.ic27" size="2097152" crc="bd6ce0ec" sha1="3d1ce5cb6978afe57967d8b53bc969259dd64749"/>
		<rom name="hotd2biosproto.ic27" size="2097152" crc="ea74e967" sha1="e4d037480eb6555d335a8ab9cd6c56122335586d"/>
		<rom name="main_eeprom.bin" size="128" crc="fea29cbb" sha1="4099f1747aafa07db34f6e072cd9bfaa83bae10e"/>
		<rom name="x76f100_eeprom.bin" size="132" crc="3ea24b6a" sha1="3a730ebcf56e0060fef6b1b02eb2eb7cfb7e61dc"/>
		<device_ref name="sh4le"/>
		<device_ref name="timer"/>
		<device_ref name="dc_g2if"/>
		<device_ref name="arm7_le"/>
		<device_ref name="maple_dc"/>
		<device_ref name="screen"/>
		<device_ref name="powervr2"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="aica"/>
		<device_ref name="aicartc"/>
		<device_ref name="93c46_16"/>
		<device_ref name="mie"/>
		<device_ref name="z80"/>
		<device_ref name="mie_jvs"/>
		<device_ref name="jvs13551"/>
		<device_ref name="tmp90ph44"/>
		<device_ref name="93c46_8"/>
		<device_ref name="x76f100"/>
		<device_ref name="m3comm"/>
		<device_ref name="m68000"/>
		<device_ref name="ram"/>
		<device_ref name="nvram"/>
		<device_ref name="naomi_rom_board"/>
	</machine>
	<machine name="isgsm" sourcefile="sega/segas16b_isgsm.cpp" isbios="yes" runnable="no">
		<description>ISG Selection Master Type 2006 BIOS</description>
		<year>2006</year>
		<manufacturer>bootleg (ISG)</manufacturer>
		<rom name="ism2006v00.u1" size="131072" crc="2292585c" sha1="97ba0e0f0be832a5114d95151e519bc027f6675b"/>
		<device_ref name="z80"/>
		<device_ref name="nvram"/>
		<device_ref name="gfxdecode"/>
		<device_ref name="palette"/>
		<device_ref name="screen"/>
		<device_ref name="sega_sys16b_sprite"/>
		<device_ref name="segaic16_video"/>
		<device_ref name="speaker"/>
		<device_ref name="ym2151"/>
		<device_ref name="upd7759"/>
		<device_ref name="netlist_sound"/>
		<device_ref name="nl_stream_in"/>
		<device_ref name="nl_stream_in"/>
		<device_ref name="nl_stream_in"/>
		<device_ref name="nl_stream_out"/>
		<device_ref name="m68000"/>
		<device_ref name="generic_latch_8"/>
	</machine>
	<machine name="iteagle" sourcefile="itech/iteagle.cpp" isbios="yes" runnable="no">
		<description>Eagle BIOS</description>
		<year>2000</year>
		<manufacturer>Incredible Technologies</manufacturer>
		<biosset name="209" description="bootrom 2.09"/>
		<biosset name="208" description="bootrom 2.08"/>
		<biosset name="204" description="bootrom 2.04"/>
		<biosset name="201" description="bootrom 2.01"/>
		<biosset name="107" description="bootrom 1.07"/>
		<biosset name="106a" description="bootrom 1.06a"/>
		<biosset name="106" description="bootrom 1.06"/>
		<biosset name="105" description="bootrom 1.05"/>
		<biosset name="103" description="bootrom 1.03"/>
		<biosset name="102" description="bootrom 1.02"/>
		<biosset name="101" description="bootrom 1.01"/>
		<rom name="17s20lpc_sb4.u26" size="32768" crc="62c4af8a" sha1="6eca277b9c66a401990599e98fdca64a9e38cc9a"/>
		<rom name="17s20lpc_sb5.u26" size="32768" crc="c88b9d42" sha1="b912d0fc50ecdc6a198c626f6e1644e8405fac6e"/>
		<rom name="17s50a_red1.u26" size="131072" crc="f5cf3187" sha1="83b4a14de9959e5a776d97d424945d43501bda7f"/>
		<rom name="e2-card1.u22.jed" size="3025" crc="9d1e1ace" sha1="287d6a30e9f32137ef4eba54f0effa092c97a6eb"/>
		<rom name="e2-res3.u117.jed" size="3025" crc="4f1ff45a" sha1="213cbdd6cd37ad9b5bfc9545084892a68d29f5ff"/>
		<rom name="eagle101.u15" size="1048576" crc="2600bc2b" sha1="c4b89e69c51e4a3bb1874407c4d30b6caed4f396"/>
		<rom name="eagle102.u15" size="1048576" crc="1fd39e73" sha1="d1ac758f94defc5c55c62594b3999a406dd9ef1f"/>
		<rom name="eagle103.u15" size="1048576" crc="c35f4cf2" sha1="45301c18c7f8f78754c8ad60ea4d2da5a7dc55fb"/>
		<rom name="eagle105.u15" size="1048576" crc="3870dbe0" sha1="09be2d86c7259cd81d945c757044b167a76f30db"/>
		<rom name="eagle106.u15" size="1048576" crc="56bc193d" sha1="e531d208ef27f777d0784414885f390d1be654b9"/>
		<rom name="eagle106a.u15" size="1048576" crc="9c79b7ad" sha1="ccf1c86e79d65bee30f399e0fa33a7839570d93b"/>
		<rom name="eagle107.u15" size="1048576" crc="97a01fc9" sha1="a421dbf4d097b2f50cc005d3cd0d63e562e03df8"/>
		<rom name="eagle201.u15" size="1048576" crc="e180442b" sha1="4f50821fed5bcd786d989520aa2559d6c416fb1f"/>
		<rom name="eagle204.u15" size="1048576" crc="f02e5523" sha1="b979cf72a6992f1ecad9695a08c8d51e315ab537"/>
		<rom name="eagle208.u15" size="1048576" crc="772f2864" sha1="085063a4e34f29ebe3814823cd2c6323a050da36"/>
		<rom name="eagle209.u15" size="1048576" crc="e0fc1a16" sha1="c9524f7ee6b95bd484a3b75bcbe2243cb273f84c"/>
		<device_ref name="vr4310le"/>
		<device_ref name="pci_root"/>
		<device_ref name="vrc4373"/>
		<device_ref name="iteagle_periph"/>
		<device_ref name="nvram"/>
		<device_ref name="ide_pci"/>
		<device_ref name="idectrl32bm"/>
		<device_ref name="ata_slot"/>
		<device_ref name="idehd"/>
		<device_ref name="harddisk_image"/>
		<device_ref name="ata_slot"/>
		<device_ref name="cdrom"/>
		<device_ref name="cdrom_image"/>
		<device_ref name="cdda"/>
		<device_ref name="idectrl32bm"/>
		<device_ref name="ata_slot"/>
		<device_ref name="idehd"/>
		<device_ref name="harddisk_image"/>
		<device_ref name="ata_slot"/>
		<device_ref name="cdrom"/>
		<device_ref name="cdrom_image"/>
		<device_ref name="cdda"/>
		<device_ref name="iteagle_fpga"/>
		<device_ref name="nvram"/>
		<device_ref name="nvram"/>
		<device_ref name="scc85c30"/>
		<device_ref name="z80scc_channel"/>
		<device_ref name="z80scc_channel"/>
		<device_ref name="rs232"/>
		<device_ref name="rs232"/>
		<device_ref name="es1373"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="voodoo_3_pci"/>
		<device_ref name="voodoo_3"/>
		<device_ref name="iteagle_eeprom"/>
		<device_ref name="93c46_16"/>
		<device_ref name="screen"/>
	</machine>
	<machine name="konamigv" sourcefile="konami/konamigv.cpp" isbios="yes" runnable="no">
		<description>Baby Phoenix-GV System</description>
		<year>1995</year>
		<manufacturer>Konami</manufacturer>
		<rom name="999a01.7e" size="524288" crc="ad498d2d" sha1="02a82a2fe1fba0404517c3602324bfa64e23e478"/>
		<device_ref name="cxd8530bq"/>
		<device_ref name="psxirq"/>
		<device_ref name="psxdma"/>
		<device_ref name="psxmdec"/>
		<device_ref name="psxrcnt"/>
		<device_ref name="psxsio0"/>
		<device_ref name="psxsio1"/>
		<device_ref name="ram"/>
		<device_ref name="mb89371"/>
		<device_ref name="93c46_16"/>
		<device_ref name="nscsi_bus"/>
		<device_ref name="nscsi_connector"/>
		<device_ref name="nxm5401"/>
		<device_ref name="cdrom_image"/>
		<device_ref name="cdda"/>
		<device_ref name="nscsi_connector"/>
		<device_ref name="ncr53cf96"/>
		<device_ref name="cxd8514q"/>
		<device_ref name="screen"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="psxspu"/>
	</machine>
	<machine name="konamigx" sourcefile="konami/konamigx.cpp" isbios="yes" runnable="no">
		<description>System GX</description>
		<year>1994</year>
		<manufacturer>Konami</manufacturer>
		<rom name="300a01.34k" size="131072" crc="d5fa95f5" sha1="c483aa98ff8ef40cdac359c19ad23fea5ecc1906"/>
		<device_ref name="m68ec020"/>
		<device_ref name="m68000"/>
		<device_ref name="tms57002"/>
		<device_ref name="k053252"/>
		<device_ref name="93c46_16"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
		<device_ref name="k056832"/>
		<device_ref name="k055555"/>
		<device_ref name="k054338"/>
		<device_ref name="k055673"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="k056800"/>
		<device_ref name="k054539"/>
		<device_ref name="k054539"/>
	</machine>
	<machine name="konendev" sourcefile="konami/konendev.cpp" isbios="yes" runnable="no">
		<description>Konami Endeavour BIOS</description>
		<year>200?</year>
		<manufacturer>Konami</manufacturer>
		<rom name="2v02s502_ifu.u190" size="524288" crc="36122a98" sha1="3d2c40c9d504358d890364e26c9562e40314d8a4"/>
		<device_ref name="ppc403gcx"/>
		<device_ref name="h83007"/>
		<device_ref name="h8h_intc"/>
		<device_ref name="h8_adc_3006"/>
		<device_ref name="h8_digital_port"/>
		<device_ref name="h8_digital_port"/>
		<device_ref name="h8_digital_port"/>
		<device_ref name="h8_digital_port"/>
		<device_ref name="h8_digital_port"/>
		<device_ref name="h8_digital_port"/>
		<device_ref name="h8_digital_port"/>
		<device_ref name="h8h_timer8_channel"/>
		<device_ref name="h8h_timer8_channel"/>
		<device_ref name="h8h_timer8_channel"/>
		<device_ref name="h8h_timer8_channel"/>
		<device_ref name="h8_timer16"/>
		<device_ref name="h8h_timer16_channel"/>
		<device_ref name="h8h_timer16_channel"/>
		<device_ref name="h8h_timer16_channel"/>
		<device_ref name="h8_sci"/>
		<device_ref name="h8_sci"/>
		<device_ref name="h8_sci"/>
		<device_ref name="h8_watchdog"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="cy7c131"/>
		<device_ref name="palette"/>
		<device_ref name="screen"/>
		<device_ref name="k057714"/>
		<device_ref name="rtc62423"/>
		<device_ref name="nvram"/>
		<device_ref name="nvram"/>
		<device_ref name="93c56_16"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="ymz280b"/>
	</machine>
	<machine name="kpython" sourcefile="konami/kpython.cpp" isbios="yes" runnable="no">
		<description>Konami Python BIOS</description>
		<year>2002</year>
		<manufacturer>Konami</manufacturer>
		<rom name="b22a01.u42" size="524288" crc="98de405e" sha1="4bc268a996825c1bdf6ae277d331fe7bdc0cc00c"/>
		<rom name="hd64f3664" size="32768" status="nodump"/>
		<device_ref name="r5900be"/>
		<device_ref name="sonyvu0"/>
		<device_ref name="sonyvu1"/>
		<device_ref name="ps2vif1"/>
		<device_ref name="ps2intc"/>
		<device_ref name="ps2gs"/>
		<device_ref name="ps2gif"/>
		<device_ref name="ps2dmac"/>
		<device_ref name="ps2sif"/>
		<device_ref name="m48t58"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
	</machine>
	<machine name="kpython2" sourcefile="konami/kpython2.cpp" isbios="yes" runnable="no">
		<description>Konami Python 2 BIOS</description>
		<year>2005</year>
		<manufacturer>Konami</manufacturer>
		<rom name="ps2-0190j-20030822.bin" size="4194304" crc="79d60546" sha1="0ea98a25a32145dda514de2f0d4bfbbd806bd00c"/>
		<device_ref name="r5900le"/>
		<device_ref name="sonyvu0"/>
		<device_ref name="sonyvu1"/>
		<device_ref name="ps2vif1"/>
		<device_ref name="ps2timer"/>
		<device_ref name="ps2timer"/>
		<device_ref name="ps2timer"/>
		<device_ref name="ps2timer"/>
		<device_ref name="ps2intc"/>
		<device_ref name="ps2gs"/>
		<device_ref name="ps2gif"/>
		<device_ref name="ps2dmac"/>
		<device_ref name="ps2sif"/>
		<device_ref name="sonyiop"/>
		<device_ref name="ps2pad"/>
		<device_ref name="ps2pad"/>
		<device_ref name="ps2mc"/>
		<device_ref name="iopintc"/>
		<device_ref name="iopsio2"/>
		<device_ref name="iopcdvd"/>
		<device_ref name="ioptimer"/>
		<device_ref name="iopspu"/>
		<device_ref name="iopdma"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
		<device_ref name="software_list"/>
	</machine>
	<machine name="kviper" sourcefile="konami/viper.cpp" isbios="yes" runnable="no">
		<description>Konami Viper BIOS</description>
		<year>1999</year>
		<manufacturer>Konami</manufacturer>
		<biosset name="bios0" description="GM941B01 (01/15/01)"/>
		<biosset name="bios1" description="GM941A01 (03/10/00)"/>
		<rom name="941a01.u25" size="262144" crc="df6f88d6" sha1="2bc10e4fbec36573aa8b6878492d37665f074d87"/>
		<rom name="941b01.u25" size="262144" crc="233e5159" sha1="66ff268d5bf78fbfa48cdc3e1b08f8956cfd6cfb"/>
		<rom name="ds2430.u3" size="40" crc="f1511505" sha1="ed7cd9b2763b3e377df9663943160f9871f65105"/>
		<device_ref name="mpc8240"/>
		<device_ref name="ds2430a"/>
		<device_ref name="pci_bus_legacy"/>
		<device_ref name="ata_interface"/>
		<device_ref name="ata_slot"/>
		<device_ref name="idehd"/>
		<device_ref name="harddisk_image"/>
		<device_ref name="ata_slot"/>
		<device_ref name="pc16552d"/>
		<device_ref name="ns16550"/>
		<device_ref name="ns16550"/>
		<device_ref name="k056230_viper"/>
		<device_ref name="voodoo_3"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="dmadac"/>
		<device_ref name="dmadac"/>
		<device_ref name="m48t58"/>
		<device_ref name="timer"/>
	</machine>
	<machine name="lindbios" sourcefile="sega/lindbergh.cpp" isbios="yes" runnable="no">
		<description>Sega Lindbergh BIOS</description>
		<year>2005</year>
		<manufacturer>Sega</manufacturer>
		<biosset name="bios0" description="6.0.0010 alternate version"/>
		<biosset name="bios1" description="6.0.0009"/>
		<biosset name="bios2" description="6.0.0010"/>
		<rom name="6.0.0009.bin" size="1048576" crc="5ffdfbf8" sha1="605bc4967b749b4e6d13fc2ebb845ba956a259a7"/>
		<rom name="6.0.0010.bin" size="1048576" crc="ea2bf888" sha1="c9c5b6f0d4f4f36620939b15dd2f128a74347e37"/>
		<rom name="6.0.0010a.bin" size="1048576" crc="10dd9b76" sha1="1fdf1f921bc395846a7c3180fbdbc4ca287a9670"/>
		<rom name="fpr-24370b.ic6" size="4194304" crc="c3b021a4" sha1="1b6938a50fe0e4ae813864649eb103838c399ac0"/>
		<rom name="vid_bios.u504" size="65536" crc="f78d14d7" sha1="f129787e487984edd23bf344f2e9500c85052275"/>
		<disk name="mda-c0004a_revb_lindyellow_v2.4.20_mvl31a_boot_2.01" sha1="e13da5f827df852e742b594729ee3f933b387410" region="cf"/>
		<device_ref name="pentium4"/>
		<device_ref name="pci_root"/>
		<device_ref name="i82875p_host"/>
		<device_ref name="i82875p_agp"/>
		<device_ref name="geforce_7600gs"/>
		<device_ref name="screen"/>
		<device_ref name="nvidia_nv3_vga"/>
		<device_ref name="i82875p_overflow"/>
		<device_ref name="pci_bridge"/>
		<device_ref name="i82541_device"/>
		<device_ref name="usb_uhci"/>
		<device_ref name="usb_uhci"/>
		<device_ref name="i6300esb_watchdog"/>
		<device_ref name="apic"/>
		<device_ref name="usb_ehci"/>
		<device_ref name="pci_bridge"/>
		<device_ref name="sb0400"/>
		<device_ref name="lindbergh_baseboard"/>
		<device_ref name="i6300esb_lpc"/>
		<device_ref name="lpc_acpi"/>
		<device_ref name="lpc_rpc"/>
		<device_ref name="lpc_pit"/>
		<device_ref name="sata"/>
		<device_ref name="smbus"/>
		<device_ref name="ac97"/>
	</machine>
	<machine name="mac2bios" sourcefile="seta/macs.cpp" isbios="yes" runnable="no">
		<description>Multi Amenity Cassette System 2 BIOS</description>
		<year>1995</year>
		<manufacturer>I'Max</manufacturer>
		<rom name="macs2os_h.bin" size="524288" status="nodump"/>
		<rom name="macs2os_l.bin" size="524288" status="nodump"/>
		<device_ref name="st0016_cpu"/>
		<device_ref name="palette"/>
		<device_ref name="st0016"/>
		<device_ref name="screen"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="generic_rom_plain"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="generic_rom_plain"/>
		<device_ref name="speaker"/>
	</machine>
	<machine name="macsbios" sourcefile="seta/macs.cpp" isbios="yes" runnable="no">
		<description>Multi Amenity Cassette System BIOS</description>
		<year>1995</year>
		<manufacturer>I'Max</manufacturer>
		<rom name="am_macs_os_hi.u44" size="524288" crc="538b68e4" sha1="a0534147791e94e726f49451d0e95671ae0a87d5"/>
		<rom name="am_macs_os_low.u43" size="524288" crc="0b5aed5e" sha1="042e705017ee34656e2c6af45825bb2dd3447747"/>
		<rom name="sx011-01.bin" size="343" crc="669096c1" sha1="36f55a2e4865bdf0506746a4df51bfb1944f905e"/>
		<device_ref name="st0016_cpu"/>
		<device_ref name="palette"/>
		<device_ref name="st0016"/>
		<device_ref name="screen"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="generic_rom_plain"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="generic_rom_plain"/>
		<device_ref name="speaker"/>
	</machine>
	<machine name="maxaflex" sourcefile="atari/maxaflex.cpp" isbios="yes" runnable="no">
		<description>Max-A-Flex</description>
		<year>1984</year>
		<manufacturer>Exidy</manufacturer>
		<rom name="atarixl.rom" size="16384" crc="1f9cd270" sha1="ae4f523ba08b6fd59f3cae515a2b2410bbd98f55"/>
		<rom name="maxaflex.uc" size="2048" crc="fe9cf53c" sha1="4b02bc2f0c8a1eab799814fac82d5812c0160206"/>
		<rom name="maxprom.prm" size="512" crc="edf5c950" sha1="9ad046ea41a61585dd8d2f2d4167a3cc39d2928f"/>
		<device_ref name="m6502"/>
		<device_ref name="timer"/>
		<device_ref name="ipt_merge_any_hi"/>
		<device_ref name="m68705p3"/>
		<device_ref name="gtia"/>
		<device_ref name="antic"/>
		<device_ref name="pia6821"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
		<device_ref name="pwm_display"/>
		<device_ref name="speaker"/>
		<device_ref name="pokey"/>
		<device_ref name="speaker_sound_device"/>
		<device_ref name="ram"/>
	</machine>
	<machine name="megaplay" sourcefile="sega/megaplay.cpp" isbios="yes" runnable="no">
		<description>Mega Play BIOS</description>
		<year>1993</year>
		<manufacturer>Sega</manufacturer>
		<biosset name="ver1" description="Mega Play BIOS (Ver. 1)"/>
		<biosset name="ver2" description="Mega Play BIOS (Ver. 2)"/>
		<rom name="315-5349a.ic54" size="260" crc="825ea316" sha1="f49edb6a3f9349330f7ff525ef60517ed276a663" status="baddump"/>
		<rom name="315-5651.ic8" size="279" crc="55c6cddb" sha1="e1a968305ca7ea17e9021b31506ca087b84a8ab1" status="baddump"/>
		<rom name="315-5653.ic56" size="279" crc="fd5c4fb3" sha1="6b2ba657836f3031d77602526416200e31d41a6e" status="baddump"/>
		<rom name="315-5654.ic33" size="260" status="nodump"/>
		<rom name="315-5655.ic34" size="260" crc="4a2d27d1" sha1="ba79183e4b522d1b57a46a56fc7d9b85de24df36" status="baddump"/>
		<rom name="315-5661.ic7" size="279" crc="d8289e31" sha1="a0e9134d9e8043a3660a2ce122cfd5d7f76773b9" status="baddump"/>
		<rom name="ep15294.ic2" size="131072" crc="aa8dc2d8" sha1="96771ad7b79dc9c83a1594243250d65052d23176"/>
		<rom name="epr-a15294.ic2" size="131072" crc="f97c68aa" sha1="bcabc879950bca1ced11c550a484e697ec5706b2"/>
		<device_ref name="m68000"/>
		<device_ref name="timer"/>
		<device_ref name="sega315_5313"/>
		<device_ref name="palette"/>
		<device_ref name="segapsg"/>
		<device_ref name="palette"/>
		<device_ref name="palette"/>
		<device_ref name="palette"/>
		<device_ref name="screen"/>
		<device_ref name="z80"/>
		<device_ref name="ipt_merge_any_hi"/>
		<device_ref name="megadrive_io_port"/>
		<device_ref name="megadrive_io_port"/>
		<device_ref name="megadrive_io_port"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="ym2612"/>
		<device_ref name="z80"/>
		<device_ref name="cxd1095"/>
		<device_ref name="cxd1095"/>
		<device_ref name="sega315_5246"/>
		<device_ref name="palette"/>
		<device_ref name="segapsg"/>
	</machine>
	<machine name="megatech" sourcefile="sega/megatech.cpp" isbios="yes" runnable="no">
		<description>Mega-Tech</description>
		<year>1989</year>
		<manufacturer>Sega</manufacturer>
		<biosset name="ver1" description="Ver 1"/>
		<biosset name="ver0a" description="Ver 0 Rev A"/>
		<biosset name="ver0b" description="Ver 0 Rev B"/>
		<biosset name="ver0aa" description="Ver 0 Rev B (alt?)"/>
		<rom name="epr-12263a.20" size="32768" crc="07c3f423" sha1="50c28bbc2d4349c820d988ae3f20aae3f808545f"/>
		<rom name="epr-12263b.20" size="32768" crc="ca26c87a" sha1="987a18bede6e54cd73c4434426eb6c302a37cdc5"/>
		<rom name="epr-12604a.20" size="32768" crc="884e4aa5" sha1="c9008c431a937c084fb475273093ca0b434b5f47"/>
		<rom name="epr-12664.20" size="32768" crc="f71e9526" sha1="1c7887541d02c41426992d17f8e3db9e03975953"/>
		<device_ref name="m68000"/>
		<device_ref name="timer"/>
		<device_ref name="sega315_5313"/>
		<device_ref name="palette"/>
		<device_ref name="segapsg"/>
		<device_ref name="palette"/>
		<device_ref name="palette"/>
		<device_ref name="palette"/>
		<device_ref name="screen"/>
		<device_ref name="z80"/>
		<device_ref name="ipt_merge_any_hi"/>
		<device_ref name="megadrive_io_port"/>
		<device_ref name="megadrive_io_port"/>
		<device_ref name="megadrive_io_port"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="ym2612"/>
		<device_ref name="z80"/>
		<device_ref name="cxd1095"/>
		<device_ref name="cxd1095"/>
		<device_ref name="screen"/>
		<device_ref name="sega315_5246"/>
		<device_ref name="palette"/>
		<device_ref name="segapsg"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="software_list"/>
	</machine>
	<machine name="naomi" sourcefile="sega/naomi.cpp" isbios="yes" runnable="no">
		<description>NAOMI BIOS</description>
		<year>1998</year>
		<manufacturer>Sega</manufacturer>
		<biosset name="bios0" description="epr-21576h (Japan)"/>
		<biosset name="bios1" description="epr-21576g (Japan)"/>
		<biosset name="bios2" description="epr-21576e (Japan)"/>
		<biosset name="bios3" description="epr-21576d (Japan)"/>
		<biosset name="bios4" description="epr-21576c (Japan)"/>
		<biosset name="bios5" description="epr-21576b (Japan)"/>
		<biosset name="bios6" description="epr-21576a (Japan)"/>
		<biosset name="bios7" description="epr-21576 (Japan)"/>
		<biosset name="bios8" description="epr-21578h (Export)"/>
		<biosset name="bios9" description="epr-21578g (Export)"/>
		<biosset name="bios10" description="epr-21578f (Export)"/>
		<biosset name="bios11" description="epr-21578e (Export)"/>
		<biosset name="bios12" description="epr-21578d (Export)"/>
		<biosset name="bios13" description="epr-21578a (Export)"/>
		<biosset name="bios14" description="epr-21577h (USA)"/>
		<biosset name="bios15" description="epr-21577g (USA)"/>
		<biosset name="bios16" description="epr-21577e (USA)"/>
		<biosset name="bios17" description="epr-21577d (USA)"/>
		<biosset name="bios18" description="epr-21577a (USA)"/>
		<biosset name="bios19" description="epr-21579d (Korea)"/>
		<biosset name="bios20" description="epr-21579 (Korea)"/>
		<biosset name="bios21" description="Set4 Dev BIOS"/>
		<biosset name="bios22" description="Dev BIOS v1.10"/>
		<biosset name="bios23" description="Dev BIOS (Nov 1998)"/>
		<biosset name="bios24" description="Development ROM Board"/>
		<biosset name="bios25" description="epr-21576h (multi-region hack)"/>
		<biosset name="bios26" description="Dev BIOS v1.2"/>
		<biosset name="bios27" description="Dev Naomi Boot 2491"/>
		<rom name="315-6188.ic31" size="8244" crc="7c9fea46" sha1="f77c07ae65dfed18c1c4c632c8945be21d02ddaf"/>
		<rom name="boot_rom_64b8.ic606" size="524288" crc="7a50fab9" sha1="ef79f448e0bf735d1264ad4f051d24178822110f"/>
		<rom name="develop.ic27" size="2097152" crc="309a196a" sha1="409b50371feb648f10efd6b7ac420bf08d9a3b5a"/>
		<rom name="develop110.ic27" size="2097152" crc="de7cfdb0" sha1="da16800edc4d49f70481c124d487f544c2fa8ce7"/>
		<rom name="epr-21336a.ic27" size="2097152" crc="d3d57af8" sha1="0eb72c2a20ad8b86d442b77760eab5e89521d469" status="baddump"/>
		<rom name="epr-21576.ic27" size="2097152" crc="9dad3495" sha1="5fb66f9a2b68d120f059c72758e65d34f461044a"/>
		<rom name="epr-21576a.ic27" size="2097152" crc="cedfe439" sha1="f27798bf3d890863ef0c1d9dcb4e7782249dca27"/>
		<rom name="epr-21576b.ic27" size="2097152" crc="755a6e07" sha1="7e8b8ccfc063144d89668e7224dcd8a36c54f3b3"/>
		<rom name="epr-21576c.ic27" size="2097152" crc="4599ad13" sha1="7e730e9452a792d76f210c33a955d385538682c7" status="baddump"/>
		<rom name="epr-21576d.ic27" size="2097152" crc="3b2afa7b" sha1="d007e1d321c198a38c5baff86eb2ab84385d150a"/>
		<rom name="epr-21576e.ic27" size="2097152" crc="08c0add7" sha1="e7c1a7673cb2ccb21748ef44105e46d1bad7266d"/>
		<rom name="epr-21576g.ic27" size="2097152" crc="d2a1c6bf" sha1="6d27d71aec4dfba98f66316ae74a1426d567698a"/>
		<rom name="epr-21576h.ic27" size="2097152" crc="d4895685" sha1="91424d481ff99a8d3f4c45cea6d3f0eada049a6d"/>
		<rom name="epr-21576h_multi.ic27" size="2097152" crc="cce01f1f" sha1="cca17119ad13e3a4ef7cb6902a37b65d6a844aee"/>
		<rom name="epr-21577a.ic27" size="2097152" crc="969dc491" sha1="581d1eae328b87b67508a7586ffc60cee256f70f"/>
		<rom name="epr-21577d.ic27" size="2097152" crc="60ddcbbe" sha1="58b15096d269d6df617ca1810b66b47deb184958"/>
		<rom name="epr-21577e.ic27" size="2097152" crc="cf36e97b" sha1="b085305982e7572e58b03a9d35f17ae319c3bbc6"/>
		<rom name="epr-21577g.ic27" size="2097152" crc="25f64af7" sha1="99f9e6cc0642319bd2da492611220540add573e8"/>
		<rom name="epr-21577h.ic27" size="2097152" crc="fdf17452" sha1="5f3e4b677f0046ce690a4f096b0481e5dd8bb6e6"/>
		<rom name="epr-21578a.ic27" size="2097152" crc="6c9aad83" sha1="555918de76d8dbee2a97d8a95297ef694b3e803f"/>
		<rom name="epr-21578d.ic27" size="2097152" crc="dfd5f42a" sha1="614a0db4743a5e5a206190d6786ade24325afbfd"/>
		<rom name="epr-21578e.ic27" size="2097152" crc="087f09a3" sha1="0418eb2cf9766f0b1b874a4e92528779e22c0a4a"/>
		<rom name="epr-21578f.ic27" size="2097152" crc="628a27fd" sha1="dae7add616b1a2478f00608823e88c3b82a0e78f"/>
		<rom name="epr-21578g.ic27" size="2097152" crc="55413214" sha1="bd2748365a9fc1821c9369aa7155d7c41c4df43e"/>
		<rom name="epr-21578h.ic27" size="2097152" crc="7b452946" sha1="8e9f153bbada24b37066dc45b64a7bf0d4f26a9b"/>
		<rom name="epr-21579.ic27" size="2097152" crc="71f9c918" sha1="d15af8b947f41eea7c203b565cd403e3f37a2017"/>
		<rom name="epr-21579d.ic27" size="2097152" crc="33513691" sha1="b1d8c7c516e1471a788fcf7a02a794ad2f05aeeb"/>
		<rom name="main_eeprom.bin" size="128" crc="fea29cbb" sha1="4099f1747aafa07db34f6e072cd9bfaa83bae10e"/>
		<rom name="naomi_boot_2491.ic27" size="2097152" crc="5b28f868" sha1="d101f58c69d9835e87a969688e43dc9b699b89d0"/>
		<rom name="x76f100_eeprom.bin" size="132" crc="3ea24b6a" sha1="3a730ebcf56e0060fef6b1b02eb2eb7cfb7e61dc"/>
		<rom name="zukinver0930.ic25" size="2097152" crc="58e17c23" sha1="19330f906accf1b859f56bbcedc2edff73747599"/>
		<device_ref name="sh4le"/>
		<device_ref name="timer"/>
		<device_ref name="dc_g2if"/>
		<device_ref name="arm7_le"/>
		<device_ref name="maple_dc"/>
		<device_ref name="screen"/>
		<device_ref name="powervr2"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="aica"/>
		<device_ref name="aicartc"/>
		<device_ref name="93c46_16"/>
		<device_ref name="mie"/>
		<device_ref name="z80"/>
		<device_ref name="mie_jvs"/>
		<device_ref name="jvs13551"/>
		<device_ref name="tmp90ph44"/>
		<device_ref name="93c46_8"/>
		<device_ref name="x76f100"/>
		<device_ref name="m3comm"/>
		<device_ref name="m68000"/>
		<device_ref name="ram"/>
		<device_ref name="nvram"/>
		<device_ref name="naomi_rom_board"/>
	</machine>
	<machine name="naomi2" sourcefile="sega/naomi.cpp" isbios="yes" runnable="no">
		<description>NAOMI 2 BIOS</description>
		<year>2001</year>
		<manufacturer>Sega</manufacturer>
		<biosset name="bios0" description="epr-23605c (Japan)"/>
		<biosset name="bios1" description="epr-23605b (Japan)"/>
		<biosset name="bios2" description="epr-23605a (Japan)"/>
		<biosset name="bios3" description="epr-23605 (Japan)"/>
		<biosset name="bios4" description="epr-23608c (Export)"/>
		<biosset name="bios5" description="epr-23608b (Export)"/>
		<biosset name="bios6" description="epr-23608a (Export)"/>
		<biosset name="bios7" description="epr-23608 (Export)"/>
		<biosset name="bios8" description="epr-23607c (USA)"/>
		<biosset name="bios9" description="epr-23607b (USA)"/>
		<biosset name="bios10" description="epr-23607 (USA)"/>
		<biosset name="bios11" description="epr-23609b (Korea)"/>
		<biosset name="bios12" description="epr-23605c (multi-region hack)"/>
		<rom name="epr-23605.ic27" size="2097152" crc="5731e446" sha1="787b0844fc408cf124c12405c095c59948709ea6"/>
		<rom name="epr-23605a.ic27" size="2097152" crc="7bc3fc2d" sha1="a4a9531a7c66ff30046908cf71f6c7b6fb59c392"/>
		<rom name="epr-23605b.ic27" size="2097152" crc="3a3242d4" sha1="aaca4df51ef91d926f8191d372f3dfe1d20d9484"/>
		<rom name="epr-23605c.ic27" size="2097152" crc="297ea6ed" sha1="cfbfe57c80e6ee86a101fa83aec0a01e00c0f42a"/>
		<rom name="epr-23605c_multi.ic27" size="2097152" crc="353fdbcd" sha1="a8b7dce572b74e02e65cb949b2c366c87625157f"/>
		<rom name="epr-23607.ic27" size="2097152" crc="2b55add2" sha1="547de5f97d3183c8cd069c4fa3c09f13d8b637d9"/>
		<rom name="epr-23607b.ic27" size="2097152" crc="f308c5e9" sha1="5470ab1cee6afecbd8ca8cf40f8fbe4ec2cb1471"/>
		<rom name="epr-23607c.ic27" size="2097152" crc="750e254b" sha1="81d0b1a076c274c6bd7c53b65e7b80e14fe039e1"/>
		<rom name="epr-23608.ic27" size="2097152" crc="929cc3a6" sha1="47d00c818de23f733a4a33b1bbc72eb8aa729246"/>
		<rom name="epr-23608a.ic27" size="2097152" crc="e8f884d1" sha1="28f4de747bb3cf860b9ebf897322fbc5d7c1e156"/>
		<rom name="epr-23608b.ic27" size="2097152" crc="a554b1e3" sha1="343b727a3619d1c75a9b6d4cc156a9050447f155"/>
		<rom name="epr-23608c.ic27" size="2097152" crc="6ef1dd8e" sha1="25ef957ec1c58fdaff5e89102002bca6c38832c5"/>
		<rom name="epr-23609b.ic27" size="2097152" crc="99e3751f" sha1="8a244f75595c49d2a37a42ab96b6bab35163ca0e"/>
		<rom name="main_eeprom.bin" size="128" crc="fea29cbb" sha1="4099f1747aafa07db34f6e072cd9bfaa83bae10e"/>
		<rom name="x76f100_eeprom.bin" size="132" crc="3ea24b6a" sha1="3a730ebcf56e0060fef6b1b02eb2eb7cfb7e61dc"/>
		<device_ref name="sh4le"/>
		<device_ref name="timer"/>
		<device_ref name="dc_g2if"/>
		<device_ref name="arm7_le"/>
		<device_ref name="maple_dc"/>
		<device_ref name="screen"/>
		<device_ref name="powervr2"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="aica"/>
		<device_ref name="aicartc"/>
		<device_ref name="93c46_16"/>
		<device_ref name="mie"/>
		<device_ref name="z80"/>
		<device_ref name="mie_jvs"/>
		<device_ref name="jvs13551"/>
		<device_ref name="tmp90ph44"/>
		<device_ref name="93c46_8"/>
		<device_ref name="x76f100"/>
		<device_ref name="m3comm"/>
		<device_ref name="m68000"/>
		<device_ref name="ram"/>
		<device_ref name="nvram"/>
		<device_ref name="naomi_rom_board"/>
	</machine>
	<machine name="naomigd" sourcefile="sega/naomi.cpp" isbios="yes" runnable="no">
		<description>NAOMI GD-ROM BIOS</description>
		<year>2001</year>
		<manufacturer>Sega</manufacturer>
		<biosset name="bios0" description="epr-21576e (Japan)"/>
		<biosset name="bios1" description="epr-21576g (Japan)"/>
		<biosset name="bios2" description="epr-21576h (Japan)"/>
		<biosset name="bios3" description="epr-21578h (Export)"/>
		<biosset name="bios4" description="epr-21578g (Export)"/>
		<biosset name="bios5" description="epr-21578e (Export)"/>
		<biosset name="bios6" description="epr-21577h (USA)"/>
		<biosset name="bios7" description="epr-21577g (USA)"/>
		<biosset name="bios8" description="epr-21577e (USA)"/>
		<rom name="epr-21576e.ic27" size="2097152" crc="08c0add7" sha1="e7c1a7673cb2ccb21748ef44105e46d1bad7266d"/>
		<rom name="epr-21576g.ic27" size="2097152" crc="d2a1c6bf" sha1="6d27d71aec4dfba98f66316ae74a1426d567698a"/>
		<rom name="epr-21576h.ic27" size="2097152" crc="d4895685" sha1="91424d481ff99a8d3f4c45cea6d3f0eada049a6d"/>
		<rom name="epr-21577e.ic27" size="2097152" crc="cf36e97b" sha1="b085305982e7572e58b03a9d35f17ae319c3bbc6"/>
		<rom name="epr-21577g.ic27" size="2097152" crc="25f64af7" sha1="99f9e6cc0642319bd2da492611220540add573e8"/>
		<rom name="epr-21577h.ic27" size="2097152" crc="fdf17452" sha1="5f3e4b677f0046ce690a4f096b0481e5dd8bb6e6"/>
		<rom name="epr-21578e.ic27" size="2097152" crc="087f09a3" sha1="0418eb2cf9766f0b1b874a4e92528779e22c0a4a"/>
		<rom name="epr-21578g.ic27" size="2097152" crc="55413214" sha1="bd2748365a9fc1821c9369aa7155d7c41c4df43e"/>
		<rom name="epr-21578h.ic27" size="2097152" crc="7b452946" sha1="8e9f153bbada24b37066dc45b64a7bf0d4f26a9b"/>
		<rom name="main_eeprom.bin" size="128" crc="fea29cbb" sha1="4099f1747aafa07db34f6e072cd9bfaa83bae10e"/>
		<rom name="x76f100_eeprom.bin" size="132" crc="3ea24b6a" sha1="3a730ebcf56e0060fef6b1b02eb2eb7cfb7e61dc"/>
		<device_ref name="sh4le"/>
		<device_ref name="timer"/>
		<device_ref name="dc_g2if"/>
		<device_ref name="arm7_le"/>
		<device_ref name="maple_dc"/>
		<device_ref name="screen"/>
		<device_ref name="powervr2"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="aica"/>
		<device_ref name="aicartc"/>
		<device_ref name="93c46_16"/>
		<device_ref name="mie"/>
		<device_ref name="z80"/>
		<device_ref name="mie_jvs"/>
		<device_ref name="jvs13551"/>
		<device_ref name="tmp90ph44"/>
		<device_ref name="93c46_8"/>
		<device_ref name="x76f100"/>
		<device_ref name="m3comm"/>
		<device_ref name="m68000"/>
		<device_ref name="ram"/>
		<device_ref name="nvram"/>
		<device_ref name="naomi_rom_board"/>
	</machine>
	<machine name="neogeo" sourcefile="neogeo/neogeo.cpp" isbios="yes" runnable="no">
		<description>Neo-Geo MV-6F</description>
		<year>1990</year>
		<manufacturer>SNK</manufacturer>
		<biosset name="euro" description="Europe MVS (Ver. 2)"/>
		<biosset name="euro-s1" description="Europe MVS (Ver. 1)"/>
		<biosset name="asia-mv1c" description="Asia NEO-MVH MV1C"/>
		<biosset name="asia-mv1b" description="Asia MV1B"/>
		<biosset name="us" description="US MVS (Ver. 2?)"/>
		<biosset name="us-e" description="US MVS (Ver. 1)"/>
		<biosset name="us-v2" description="US MVS (4 slot, Ver 2)"/>
		<biosset name="us-u4" description="US MVS (U4)"/>
		<biosset name="us-u3" description="US MVS (U3)"/>
		<biosset name="japan" description="Japan MVS (Ver. 3)"/>
		<biosset name="japan-s2" description="Japan MVS (Ver. 2)"/>
		<biosset name="japan-s1" description="Japan MVS (Ver. 1)"/>
		<biosset name="japan-mv1b" description="Japan MV1B"/>
		<biosset name="japan-j3a" description="Japan MVS (J3, alt)"/>
		<biosset name="japan-mv1c" description="Japan NEO-MVH MV1C"/>
		<biosset name="japan-hotel" description="Custom Japanese Hotel"/>
		<biosset name="unibios40" description="Universe BIOS (Hack, Ver. 4.0)"/>
		<biosset name="unibios33" description="Universe BIOS (Hack, Ver. 3.3)"/>
		<biosset name="unibios32" description="Universe BIOS (Hack, Ver. 3.2)"/>
		<biosset name="unibios31" description="Universe BIOS (Hack, Ver. 3.1)"/>
		<biosset name="unibios30" description="Universe BIOS (Hack, Ver. 3.0)"/>
		<biosset name="unibios23" description="Universe BIOS (Hack, Ver. 2.3)"/>
		<biosset name="unibios23o" description="Universe BIOS (Hack, Ver. 2.3, older?)"/>
		<biosset name="unibios22" description="Universe BIOS (Hack, Ver. 2.2)"/>
		<biosset name="unibios21" description="Universe BIOS (Hack, Ver. 2.1)"/>
		<biosset name="unibios20" description="Universe BIOS (Hack, Ver. 2.0)"/>
		<biosset name="unibios13" description="Universe BIOS (Hack, Ver. 1.3)"/>
		<biosset name="unibios12" description="Universe BIOS (Hack, Ver. 1.2)"/>
		<biosset name="unibios12o" description="Universe BIOS (Hack, Ver. 1.2, older)"/>
		<biosset name="unibios11" description="Universe BIOS (Hack, Ver. 1.1)"/>
		<biosset name="unibios10" description="Universe BIOS (Hack, Ver. 1.0)"/>
		<rom name="000-lo.lo" size="131072" crc="5a86cff2" sha1="5992277debadeb64d1c1c64b0a92d9293eaf7e4a"/>
		<rom name="japan-j3.bin" size="131072" crc="dff6d41f" sha1="e92910e20092577a4523a6b39d578a71d4de7085"/>
		<rom name="sfix.sfix" size="131072" crc="c2ea0cfd" sha1="fd4a618cdcdbf849374f0a50dd8efe9dbab706c3"/>
		<rom name="sm1.sm1" size="131072" crc="94416d67" sha1="42f9d7ddd6c0931fd64226a60dc73602b2819dcf"/>
		<rom name="sp-1v1_3db8c.bin" size="131072" crc="162f0ebe" sha1="fe1c6dd3dfcf97d960065b1bb46c1e11cb7bf271"/>
		<rom name="sp-45.sp1" size="524288" crc="03cc9f6a" sha1="cdf1f49e3ff2bac528c21ed28449cf35b7957dc1"/>
		<rom name="sp-e.sp1" size="131072" crc="2723a5b5" sha1="5dbff7531cf04886cde3ef022fb5ca687573dcb8"/>
		<rom name="sp-j2.sp1" size="131072" crc="acede59c" sha1="b6f97acd282fd7e94d9426078a90f059b5e9dd91"/>
		<rom name="sp-j3.sp1" size="524288" crc="486cb450" sha1="52c21ea817928904b80745a8c8d15cbad61e1dc1"/>
		<rom name="sp-s.sp1" size="131072" crc="c7f2fa45" sha1="09576ff20b4d6b365e78e6a5698ea450262697cd"/>
		<rom name="sp-s2.sp1" size="131072" crc="9036d879" sha1="4f5ed7105b7128794654ce82b51723e16e389543"/>
		<rom name="sp-s3.sp1" size="131072" crc="91b64be3" sha1="720a3e20d26818632aedf2c2fd16c54f213543e1"/>
		<rom name="sp-u2.sp1" size="131072" crc="e72943de" sha1="5c6bba07d2ec8ac95776aa3511109f5e1e2e92eb"/>
		<rom name="sp1-j3.bin" size="131072" crc="fbc6d469" sha1="46b2b409b5b68869e367b40c846373623edb632a"/>
		<rom name="sp1-u2" size="131072" crc="62f021f4" sha1="62d372269e1b3161c64ae21123655a0a22ffd1bb"/>
		<rom name="sp1-u3.bin" size="131072" crc="2025b7a2" sha1="73d774746196f377111cd7aa051cc8bb5dd948b3"/>
		<rom name="sp1-u4.bin" size="131072" crc="1179a30f" sha1="866817f47aa84d903d0b819d61f6ef356893d16a"/>
		<rom name="sp1.jipan.1024" size="131072" crc="9fb0abe4" sha1="18a987ce2229df79a8cf6a84f968f0e42ce4e59d"/>
		<rom name="uni-bios_1_0.rom" size="131072" crc="0ce453a0" sha1="3b4c0cd26c176fc6b26c3a2f95143dd478f6abf9"/>
		<rom name="uni-bios_1_1.rom" size="131072" crc="5dda0d84" sha1="4153d533c02926a2577e49c32657214781ff29b7"/>
		<rom name="uni-bios_1_2.rom" size="131072" crc="4fa698e9" sha1="682e13ec1c42beaa2d04473967840c88fd52c75a"/>
		<rom name="uni-bios_1_2o.rom" size="131072" crc="e19d3ce9" sha1="af88ef837f44a3af2d7144bb46a37c8512b67770"/>
		<rom name="uni-bios_1_3.rom" size="131072" crc="b24b44a0" sha1="eca8851d30557b97c309a0d9f4a9d20e5b14af4e"/>
		<rom name="uni-bios_2_0.rom" size="131072" crc="0c12c2ad" sha1="37bcd4d30f3892078b46841d895a6eff16dc921e"/>
		<rom name="uni-bios_2_1.rom" size="131072" crc="8dabf76b" sha1="c23732c4491d966cf0373c65c83c7a4e88f0082c"/>
		<rom name="uni-bios_2_2.rom" size="131072" crc="2d50996a" sha1="5241a4fb0c63b1a23fd1da8efa9c9a9bd3b4279c"/>
		<rom name="uni-bios_2_3.rom" size="131072" crc="27664eb5" sha1="5b02900a3ccf3df168bdcfc98458136fd2b92ac0"/>
		<rom name="uni-bios_2_3o.rom" size="131072" crc="601720ae" sha1="1b8a72c720cdb5ee3f1d735bbcf447b09204b8d9"/>
		<rom name="uni-bios_3_0.rom" size="131072" crc="a97c89a9" sha1="97a5eff3b119062f10e31ad6f04fe4b90d366e7f"/>
		<rom name="uni-bios_3_1.rom" size="131072" crc="0c58093f" sha1="29329a3448c2505e1ff45ffa75e61e9693165153"/>
		<rom name="uni-bios_3_2.rom" size="131072" crc="a4e8b9b3" sha1="c92f18c3f1edda543d264ecd0ea915240e7c8258"/>
		<rom name="uni-bios_3_3.rom" size="131072" crc="24858466" sha1="0ad92efb0c2338426635e0159d1f60b4473d0785"/>
		<rom name="uni-bios_4_0.rom" size="131072" crc="a7aab458" sha1="938a0bda7d9a357240718c2cec319878d36b8f72"/>
		<rom name="vs-bios.rom" size="131072" crc="f0e8f27d" sha1="ecf01eda815909f1facec62abf3594eaa8d11075"/>
		<device_ref name="m68000"/>
		<device_ref name="z80"/>
		<device_ref name="hc259"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
		<device_ref name="neosprite_opt"/>
		<device_ref name="ipt_merge_all_hi"/>
		<device_ref name="generic_latch_8"/>
		<device_ref name="generic_latch_8"/>
		<device_ref name="ym2610"/>
		<device_ref name="watchdog"/>
		<device_ref name="upd4990a"/>
		<device_ref name="nvram"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="ng_memcard"/>
		<device_ref name="neogeo_ctrl_edge"/>
		<device_ref name="neogeo_joyac"/>
		<device_ref name="neogeo_control_port"/>
		<device_ref name="neogeo_control_port"/>
		<device_ref name="neogeo_cart_slot"/>
		<device_ref name="neogeo_cart_slot"/>
		<device_ref name="neogeo_cart_slot"/>
		<device_ref name="neogeo_cart_slot"/>
		<device_ref name="neogeo_cart_slot"/>
		<device_ref name="neogeo_cart_slot"/>
		<device_ref name="software_list"/>
	</machine>
	<machine name="nichidvd" sourcefile="nichibutsu/hrdvd.cpp" isbios="yes" runnable="no">
		<description>Nichibutsu High Rate DVD BIOS</description>
		<year>1998</year>
		<manufacturer>Nichibutsu</manufacturer>
		<biosset name="vb102" description="va1b102"/>
		<biosset name="vb101" description="va1b101"/>
		<biosset name="va101" description="va1a101"/>
		<rom name="va1a101.u2" size="131072" crc="36135792" sha1="1b9c50bd02df8227b228b35cc485efd5a13ec639"/>
		<rom name="va1b101.u2" size="131072" crc="b92a83c8" sha1="bd6d9adaa74cf7512478838d1bd5a79dbd0c4aa1"/>
		<rom name="va1b102.u2" size="131072" crc="67374715" sha1="8767cbd81614c2686a1adb70159f909e8ffd634d"/>
		<device_ref name="tmp68301"/>
		<device_ref name="h83002"/>
		<device_ref name="h8h_intc"/>
		<device_ref name="h8_adc_3337"/>
		<device_ref name="h8h_dma"/>
		<device_ref name="h8h_dma_channel"/>
		<device_ref name="h8h_dma_channel"/>
		<device_ref name="h8_digital_port"/>
		<device_ref name="h8_digital_port"/>
		<device_ref name="h8_digital_port"/>
		<device_ref name="h8_digital_port"/>
		<device_ref name="h8_digital_port"/>
		<device_ref name="h8_digital_port"/>
		<device_ref name="h8_digital_port"/>
		<device_ref name="h8_timer16"/>
		<device_ref name="h8h_timer16_channel"/>
		<device_ref name="h8h_timer16_channel"/>
		<device_ref name="h8h_timer16_channel"/>
		<device_ref name="h8h_timer16_channel"/>
		<device_ref name="h8h_timer16_channel"/>
		<device_ref name="h8_sci"/>
		<device_ref name="h8_sci"/>
		<device_ref name="h8_watchdog"/>
		<device_ref name="hrdvd_atactrl"/>
		<device_ref name="ata_slot"/>
		<device_ref name="dvdrom_fixed"/>
		<device_ref name="dvdrom_image"/>
		<device_ref name="cdda"/>
		<device_ref name="ata_slot"/>
		<device_ref name="tc9223"/>
		<device_ref name="v9958"/>
		<device_ref name="screen"/>
		<device_ref name="zr36110"/>
		<device_ref name="nn71003f"/>
		<device_ref name="nichisnd"/>
		<device_ref name="tmpz84c011"/>
		<device_ref name="z80ctc"/>
		<device_ref name="z80ctc_channel"/>
		<device_ref name="z80ctc_channel"/>
		<device_ref name="z80ctc_channel"/>
		<device_ref name="z80ctc_channel"/>
		<device_ref name="speaker"/>
		<device_ref name="generic_latch_8"/>
		<device_ref name="ym3812"/>
		<device_ref name="dac_8bit_r2r"/>
		<device_ref name="dac_8bit_r2r"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
	</machine>
	<machine name="nss" sourcefile="nintendo/nss.cpp" isbios="yes" runnable="no">
		<description>Nintendo Super System BIOS</description>
		<year>199?</year>
		<manufacturer>Nintendo</manufacturer>
		<biosset name="single" description="Nintendo Super System (Single Cart BIOS)"/>
		<biosset name="multi" description="Nintendo Super System (Multi Cart BIOS)"/>
		<biosset name="single3" description="Nintendo Super System (Single Cart BIOS v3, hack?)"/>
		<rom name="nss-c.ic14" size="32768" crc="a8e202b3" sha1="b7afcfe4f5cf15df53452dc04be81929ced1efb2"/>
		<rom name="nss-ic14.02.ic14" size="32768" crc="e06cb58f" sha1="62f507e91a2797919a78d627af53f029c7d81477"/>
		<rom name="nss-v3.ic14" size="32768" crc="ac385b53" sha1="e3942f9d508c3c8074c3c3941376c37ca68b8e54"/>
		<device_ref name="5a22"/>
		<device_ref name="s_smp"/>
		<device_ref name="z80"/>
		<device_ref name="m50458"/>
		<device_ref name="s3520cf"/>
		<device_ref name="rp5h01"/>
		<device_ref name="m6m80011ap"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="s_dsp"/>
		<device_ref name="screen"/>
		<device_ref name="snes_ppu"/>
		<device_ref name="screen"/>
	</machine>
	<machine name="pgm" sourcefile="igs/pgm.cpp" isbios="yes" runnable="no">
		<description>PGM (Polygame Master) System BIOS</description>
		<year>1997</year>
		<manufacturer>IGS</manufacturer>
		<biosset name="v2" description="PGM BIOS V2"/>
		<biosset name="v1" description="PGM BIOS V1"/>
		<rom name="pgm_m01s.rom" size="2097152" crc="45ae7159" sha1="d3ed3ff3464557fd0df6b069b2e431528b0ebfa8"/>
		<rom name="pgm_p01s.u20" size="131072" crc="e42b166e" sha1="2a9df9ec746b14b74fae48b1a438da14973702ea"/>
		<rom name="pgm_p02s.u20" size="131072" crc="78c15fa2" sha1="885a6558e022602cc6f482ac9667ba9f61e75092"/>
		<rom name="pgm_t01s.rom" size="2097152" crc="1a7123a0" sha1="cc567f577bfbf45427b54d6695b11b74f2578af3"/>
		<device_ref name="m68000"/>
		<device_ref name="timer"/>
		<device_ref name="z80"/>
		<device_ref name="nvram"/>
		<device_ref name="v3021"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
		<device_ref name="speaker"/>
		<device_ref name="generic_latch_8"/>
		<device_ref name="generic_latch_8"/>
		<device_ref name="generic_latch_8"/>
		<device_ref name="igs023"/>
		<device_ref name="ics2115"/>
	</machine>
	<machine name="playch10" sourcefile="nintendo/playch10.cpp" isbios="yes" runnable="no">
		<description>PlayChoice-10 BIOS</description>
		<year>1986</year>
		<manufacturer>Nintendo of America</manufacturer>
		<biosset name="dual" description="Dual Monitor Version"/>
		<biosset name="single" description="Single Monitor Version"/>
		<biosset name="alt" description="Alternate BIOS"/>
		<biosset name="singleb" description="Single Monitor Version (Newer?)"/>
		<biosset name="dualb" description="Dual Monitor Version (alternate)"/>
		<rom name="pch1-c-6d.82s129an.6d" size="256" crc="1213ebd4" sha1="0ad386fc3eab5e53c0288ad1de33639a9e461b7c"/>
		<rom name="pch1-c-6e.82s129an.6e" size="256" crc="a2625c6e" sha1="a448b47c9289902e26a3d3c4c7d5a7968c385e81"/>
		<rom name="pch1-c-6f.82s129an.6f" size="256" crc="e5414ca3" sha1="d2878411cda84ffe0afb2e538a67457f51bebffb"/>
		<rom name="pch1-c_8m.8m" size="8192" crc="83ebc7a3" sha1="a7c607138f4f9b96ab5d3a82c47895f77672e296"/>
		<rom name="pch1-c_8p-8p" size="8192" crc="90e1b80c" sha1="c4f4b135b2a11743518aaa0554c365b4a8cf299a"/>
		<rom name="pch1-c_8te.8t" size="16384" crc="123ffa37" sha1="3bef754a5a85a8498bb6222ddf5cb9021f264db5"/>
		<rom name="pch1-c__8k.8k" size="8192" crc="9acffb30" sha1="b814f10ef23f2ca445fabafcbf7f25e2d454ba8c"/>
		<rom name="pch1-c__8m_e-1.8m" size="8192" crc="c1232eee" sha1="beaf9fa2d091a3c7f70c51e966d885b1f9f0935f"/>
		<rom name="pch1-c__8p_e-1.8p" size="8192" crc="30c15e23" sha1="69166afdb2fe827c7f1919cdf4197caccbd961fa"/>
		<rom name="pch1-c__8t_e-1.8t" size="16384" crc="88a8f87e" sha1="d1d7ffe68d2e7aa2faf8ad41a7ec8421265ede42"/>
		<rom name="pch1-c__8t_e-2.8t" size="16384" crc="d52fa07a" sha1="55cabf52ae10c050c2229081a80b9fe5454ab8c5"/>
		<rom name="pck1-c.8t" size="16384" crc="503ee8b1" sha1="3bd20bc71cac742d1b8c1430a6426d0a19db7ad0"/>
		<rom name="pck1-c_fix.8t" size="16384" crc="0be8ceb4" sha1="45b127a537370226e6b30be2b5a92ad05673ca7f"/>
		<rom name="rp2c0x.pal" size="192" crc="48de65dc" sha1="d10acafc8da9ff479c270ec01180cca61efe62f5"/>
		<device_ref name="z80"/>
		<device_ref name="rp2a03g"/>
		<device_ref name="nesapu"/>
		<device_ref name="ls259"/>
		<device_ref name="ls259"/>
		<device_ref name="gfxdecode"/>
		<device_ref name="palette"/>
		<device_ref name="screen"/>
		<device_ref name="screen"/>
		<device_ref name="ppu2c03b"/>
		<device_ref name="nes_zapper_sensor"/>
		<device_ref name="speaker"/>
		<device_ref name="rp5h01"/>
	</machine>
	<machine name="pumpitup" sourcefile="misc/xtom3d.cpp" isbios="yes" runnable="no">
		<description>Pump It Up BIOS</description>
		<year>1999</year>
		<manufacturer>Andamiro</manufacturer>
		<biosset name="mk3v10" description="mk3 v1.0"/>
		<biosset name="mk3v11" description="mk3 v1.1"/>
		<rom name="mk3_1.0_bios.u22" size="131072" crc="a2b5546b" sha1="d99d29615e2b9c8784e03d4270cf7bb6569f389d"/>
		<rom name="mk3_1.1_bios.u22" size="131072" crc="4540c23f" sha1="bba697dbe234e4f14c23aac126ea36df216f8c93"/>
		<rom name="piu10.u8" size="2097152" crc="5911e31a" sha1="295723b9b7da9e55b5dd5586b23b06355f4837ef"/>
		<rom name="piu10.u9" size="2097152" crc="9c436cfa" sha1="480ea52e74721d1963ced41be5c482b7b913ccd2"/>
		<device_ref name="pentium2"/>
		<device_ref name="pci_root"/>
		<device_ref name="i82443bx_host"/>
		<device_ref name="i82443bx_bridge"/>
		<device_ref name="banshee_x86"/>
		<device_ref name="voodoo_banshee"/>
		<device_ref name="i82371eb_isa"/>
		<device_ref name="pit8254"/>
		<device_ref name="pit_counter"/>
		<device_ref name="pit_counter"/>
		<device_ref name="pit_counter"/>
		<device_ref name="am9517a"/>
		<device_ref name="am9517a"/>
		<device_ref name="pic8259"/>
		<device_ref name="pic8259"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker_sound_device"/>
		<device_ref name="isa16"/>
		<device_ref name="i82371eb_ide"/>
		<device_ref name="idectrl32bm"/>
		<device_ref name="ata_slot"/>
		<device_ref name="cdrom"/>
		<device_ref name="cdrom_image"/>
		<device_ref name="cdda"/>
		<device_ref name="ata_slot"/>
		<device_ref name="idectrl32bm"/>
		<device_ref name="ata_slot"/>
		<device_ref name="ata_slot"/>
		<device_ref name="i82371eb_usb"/>
		<device_ref name="i82371eb_acpi"/>
		<device_ref name="lpc_acpi"/>
		<device_ref name="smbus"/>
		<device_ref name="isa16_slot"/>
		<device_ref name="isa16_piu10"/>
		<device_ref name="macronix_29f1610mc_16bit"/>
		<device_ref name="cat702_piu"/>
		<device_ref name="dac3350a"/>
		<device_ref name="mas3507d"/>
		<device_ref name="isa16_slot"/>
		<device_ref name="isa16_oksan_lpc"/>
		<device_ref name="mc146818"/>
		<device_ref name="kbdc8042"/>
		<device_ref name="isa16_slot"/>
		<device_ref name="isa16_pumpitup_io_sound"/>
		<device_ref name="93c46_16"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="ymz280b"/>
		<device_ref name="isa16_slot"/>
		<device_ref name="screen"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
	</machine>
	<machine name="recel" sourcefile="pinball/recel.cpp" sampleof="genpin" isbios="yes" runnable="no">
		<description>Recel BIOS</description>
		<year>1977</year>
		<manufacturer>Recel</manufacturer>
		<rom name="a2361.b1" size="2048" crc="d0c4695d" sha1="4846adb3f6c292626840ba5255ffc5e788a69301"/>
		<rom name="a2362.b2" size="2048" crc="39a70611" sha1="8545e168a5f256150bcff12d1e6d8efffd08c3cd"/>
		<device_ref name="pps4_2"/>
		<device_ref name="nvram"/>
		<device_ref name="ra17xx"/>
		<device_ref name="ra17xx"/>
		<device_ref name="r10696"/>
		<device_ref name="r10788"/>
		<device_ref name="speaker"/>
		<device_ref name="samples"/>
		<sample name="bumper"/>
		<sample name="chime1"/>
		<sample name="chime2"/>
		<sample name="chime3"/>
		<sample name="chime4"/>
		<sample name="coil_coinlockout_engage"/>
		<sample name="coil_coinlockout_release"/>
		<sample name="coinin"/>
		<sample name="drop_target_reset"/>
		<sample name="hole"/>
		<sample name="kickback"/>
		<sample name="knocker"/>
		<sample name="outhole"/>
		<sample name="relay_engage"/>
		<sample name="relay_release"/>
		<sample name="sling"/>
		<sample name="solenoid_engage"/>
		<sample name="solenoid_release"/>
	</machine>
	<machine name="sammymdl" sourcefile="sigma/sigmab98.cpp" isbios="yes" runnable="no">
		<description>Sammy Medal Game System BIOS</description>
		<year>2000</year>
		<manufacturer>Sammy</manufacturer>
		<biosset name="v5" description="IPL Ver. 5.0"/>
		<biosset name="v4" description="IPL Ver. 4.0"/>
		<rom name="mt201l04.u012" size="524288" crc="c8c6d25f" sha1="5be39fa72b65f2e455ccc146dbab58d24ab46505"/>
		<rom name="vm1211l01.u2" size="524288" crc="c3c74dc5" sha1="07352e6dba7514214e778ba39e1ca773e4698858"/>
		<device_ref name="kl5c80a12"/>
		<device_ref name="kp69"/>
		<device_ref name="kp64"/>
		<device_ref name="kp64"/>
		<device_ref name="kp63_3channel"/>
		<device_ref name="nvram"/>
		<device_ref name="93c46_8"/>
		<device_ref name="ticket_dispenser"/>
		<device_ref name="watchdog"/>
		<device_ref name="screen"/>
		<device_ref name="gfxdecode"/>
		<device_ref name="palette"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="okim9810"/>
	</machine>
	<machine name="segasp" sourcefile="sega/segasp.cpp" isbios="yes" runnable="no">
		<description>Sega System SP (Spider) BIOS</description>
		<year>2004</year>
		<manufacturer>Sega</manufacturer>
		<biosset name="v101" description="BOOT VER 1.01"/>
		<biosset name="v200" description="BOOT VER 2.00"/>
		<biosset name="v201" description="BOOT VER 2.01"/>
		<rom name="epr-24236a.ic50" size="2097152" crc="ca7df0de" sha1="504c74d5fc96c53ef9f7753e9e37fb8b39cb628c"/>
		<rom name="epr-24328.ic50" size="2097152" crc="25f2ef00" sha1="e58dec9f171e52b3ded213b3fcd9a0de8a438076"/>
		<rom name="epr-24328a.ic50" size="2097152" crc="03ec3805" sha1="a8fbaea826ca257be0b2b86952f247254929e046"/>
		<rom name="fpr-24208a.ic72" size="2097152" crc="a738ea1c" sha1="3c32ddfb3c40be66b9fb2ba35fbfd5b534bb3da0"/>
		<rom name="fpr-24329.ic72" size="2097152" crc="a738ea1c" sha1="d0d062a4089a2d3404df45eb015faaf7eee9b8c2"/>
		<rom name="fpr-24407.ic72" size="2097152" crc="a738ea1c" sha1="fbcc3d119b47a6da4d194e3fe4a98126c7049edf"/>
		<rom name="fpr-24407_123.ic72" size="2097152" crc="a738ea1c" sha1="3f5a2fb03bbb1bd9af9fe32ad76a224c97aa9b7a"/>
		<rom name="mb_eeprom_exp.ic54s" size="128" crc="947ddfad" sha1="832a3db097af680d1d0eb9451b4650565f0cf8c7"/>
		<rom name="mb_eeprom_us.ic54s" size="128" crc="4186d7ab" sha1="fc23da69a511a7643b6a066161bcfc3cdeeacf04"/>
		<rom name="mb_serial.ic57" size="128" crc="e1e3c009" sha1="66bc636c527389c3338f631d78c788b4bd4e93be"/>
		<rom name="net_eeprom.ic74s" size="512" crc="77cc5a6c" sha1="cbfba546256b70bce6c6fd0030d7e2e410a25526"/>
		<rom name="net_firm_119.ic72" size="2097152" crc="a738ea1c" sha1="d25187a973a7e166e70334f964363adf2be87257"/>
		<device_ref name="sh4le"/>
		<device_ref name="timer"/>
		<device_ref name="dc_g2if"/>
		<device_ref name="arm7_le"/>
		<device_ref name="maple_dc"/>
		<device_ref name="screen"/>
		<device_ref name="powervr2"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="aica"/>
		<device_ref name="aicartc"/>
		<device_ref name="93c46_16"/>
		<device_ref name="93c46_16"/>
		<device_ref name="x76f100"/>
		<device_ref name="naomi_m4_board"/>
	</machine>
	<machine name="sfcbox" sourcefile="nintendo/sfcbox.cpp" isbios="yes" runnable="no">
		<description>Super Famicom Box BIOS</description>
		<year>1994</year>
		<manufacturer>Nintendo</manufacturer>
		<biosset name="2.00" description="SFCBox BIOS Version 2.00"/>
		<biosset name="1.00" description="SFCBox BIOS Version 1.00"/>
		<rom name="atrom-4s-0.rom5" size="524288" crc="ad3ec05c" sha1="a3d336db585fe02a37c323422d9db6a33fd489a6"/>
		<rom name="krom1.ic1" size="65536" crc="c9010002" sha1="f4c74086a83b728b1c1af3a021a60efa80eff5a4"/>
		<rom name="krom2.00.ic1" size="131072" crc="e31b5580" sha1="4a6a34a9a94c8249c3b441c2516bdd03e198c458"/>
		<device_ref name="5a22"/>
		<device_ref name="s_smp"/>
		<device_ref name="z80180"/>
		<device_ref name="z180asci_channel_0"/>
		<device_ref name="z180asci_channel_1"/>
		<device_ref name="z180csio"/>
		<device_ref name="mb90082"/>
		<device_ref name="s3520cf"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="s_dsp"/>
		<device_ref name="screen"/>
		<device_ref name="snes_ppu"/>
		<device_ref name="screen"/>
	</machine>
	<machine name="shtzone" sourcefile="sega/shtzone.cpp" isbios="yes" runnable="no">
		<description>Shooting Zone System BIOS</description>
		<year>1987</year>
		<manufacturer>Sega</manufacturer>
		<rom name="epr10894a.20" size="16384" crc="ea8901d9" sha1="43fd8bfc395e3b2e3fbe9645d692a5eb04783d9c"/>
		<device_ref name="z80"/>
		<device_ref name="speaker"/>
		<device_ref name="sms_cart_slot"/>
		<device_ref name="software_list"/>
		<device_ref name="sms_control_port"/>
		<device_ref name="sms_light_phaser"/>
		<device_ref name="sms_control_port"/>
		<device_ref name="sms_light_phaser"/>
		<device_ref name="z80"/>
		<device_ref name="nvram"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
		<device_ref name="sega315_5124"/>
		<device_ref name="palette"/>
		<device_ref name="segapsg"/>
		<device_ref name="beep"/>
		<device_ref name="sms_cart_slot"/>
		<device_ref name="sms_cart_slot"/>
		<device_ref name="sms_cart_slot"/>
		<device_ref name="sms_cart_slot"/>
	</machine>
	<machine name="skns" sourcefile="kaneko/suprnova.cpp" isbios="yes" runnable="no">
		<description>Super Kaneko Nova System BIOS</description>
		<year>1996</year>
		<manufacturer>Kaneko</manufacturer>
		<biosset name="japan" description="Japan"/>
		<biosset name="europe" description="Europe"/>
		<biosset name="asia" description="Asia"/>
		<biosset name="usa" description="USA"/>
		<biosset name="korea" description="Korea"/>
		<biosset name="japanmod" description="Japan (No Region Lock)"/>
		<biosset name="koreamod" description="Korea (No Region Lock)"/>
		<rom name="sknsa1.u10" size="524288" crc="745e5212" sha1="caba649ab2d83b2d7e007eecee0fc582c019df38"/>
		<rom name="sknse2.u10" size="524288" crc="e2b9d7d1" sha1="b530a3bb9dedc8cfafcba9f1f10277590be04a15"/>
		<rom name="sknsj1.u10" size="524288" crc="7e2b836c" sha1="92c5a7a2472496028bff0e5980d41dd294f42144"/>
		<rom name="sknsk1.u10" size="524288" crc="ff1c9f79" sha1="a51e598d43e76d37da69b1f094c111273bdfc94a"/>
		<rom name="sknsu1.u10" size="524288" crc="384d21ec" sha1="a27e8a18099d9cea64fa32db28d01101c2a78815"/>
		<rom name="supernova-modbios-korea.u10" size="524288" crc="1d90517c" sha1="463962ffe19880135f0d95a7beda79e27448e872"/>
		<rom name="supernova_modbios-japan.u10" size="524288" crc="b8d3190c" sha1="62c9a4a075fd944e89fe95c6b46046101eb6de1c"/>
		<device_ref name="sh2_7604"/>
		<device_ref name="timer"/>
		<device_ref name="msm6242"/>
		<device_ref name="nvram"/>
		<device_ref name="timer"/>
		<device_ref name="timer"/>
		<device_ref name="timer"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
		<device_ref name="gfxdecode"/>
		<device_ref name="sknsspr"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="ymz280b"/>
	</machine>
	<machine name="stvbios" sourcefile="sega/stv.cpp" isbios="yes" runnable="no">
		<description>ST-V BIOS</description>
		<year>1996</year>
		<manufacturer>Sega</manufacturer>
		<biosset name="jp" description="EPR-23603 (Japan 00/10/24)"/>
		<biosset name="jp1" description="EPR-20091 (Japan 97/08/21)"/>
		<biosset name="jp2" description="EPR-19730 (Japan 97/02/17)"/>
		<biosset name="jp3" description="EPR-17951A (Japan 95/04/25)"/>
		<biosset name="jp4" description="EPR-17740A (Japan 95/02/20)"/>
		<biosset name="jp5" description="EPR-17740 (Japan 95/01/31)"/>
		<biosset name="euro" description="EPR-17954A (Europe 95/04/25)"/>
		<biosset name="us" description="EPR-17952A (USA 95/04/25)"/>
		<biosset name="us1" description="EPR-17741a (USA 95/02/20)"/>
		<biosset name="tw" description="EPR-19854 (Taiwan 97/05/15)"/>
		<biosset name="tw1" description="EPR-17953A (Taiwan 95/04/25)"/>
		<biosset name="tw2" description="EPR-17742A (Taiwan 95/02/20)"/>
		<biosset name="debug" description="Development (1.10, 95/01/13)"/>
		<biosset name="dev" description="Development (1.061, 94/11/25)"/>
		<rom name="epr-17740.ic8" size="524288" crc="5c5aa63d" sha1="06860d96923b81afbc21e0ad32ee19487d8ff6e7"/>
		<rom name="epr-17740a.ic8" size="524288" crc="3e23c81f" sha1="f9b282fd27693e9891843597b2e1823da3d23c7b"/>
		<rom name="epr-17741a.ic8" size="524288" crc="4166c663" sha1="cc41d30de06160083d77e0dc5d69e61fec7fdcb5"/>
		<rom name="epr-17742a.ic8" size="524288" crc="02daf123" sha1="23185beb1ce9c09b8719e57d1adb7b28c8141fd5"/>
		<rom name="epr-17951a.ic8" size="524288" crc="2672f9d8" sha1="63cf4a6432f6c87952f9cf3ab0f977aed2367303"/>
		<rom name="epr-17952a.ic8" size="524288" crc="d1be2adf" sha1="eaf1c3e5d602e1139d2090a78d7e19f04f916794"/>
		<rom name="epr-17953a.ic8" size="524288" crc="a4c47570" sha1="9efc73717ec8a13417e65c54344ded9fc25bf5ef"/>
		<rom name="epr-17954a.ic8" size="524288" crc="f7722da3" sha1="af79cff317e5b57d49e463af16a9f616ed1eee08"/>
		<rom name="epr-19730.ic8" size="524288" crc="d0e0889d" sha1="fae53107c894e0c41c49e191dbe706c9cd6e50bd"/>
		<rom name="epr-19854.ic8" size="524288" crc="e09d1f60" sha1="b55cdcb45b2a5b0b35e352cf7625f0bd659084df"/>
		<rom name="epr-20091.ic8" size="524288" crc="59ed40f4" sha1="eff0f54c70bce05ff3a289bf30b1027e1c8cd117"/>
		<rom name="epr-23603.ic8" size="524288" crc="f688ae60" sha1="1a31b6b1a4257fcb6ac6a91e67dd798f91505f48"/>
		<rom name="stv1061.bin" size="524288" crc="728dbca3" sha1="0ed2030177f0aa8285645c395ae9ad9f568ab1d6"/>
		<rom name="stv110.bin" size="524288" crc="3dfeda92" sha1="8eb33192a57df5f3a1dfb57263054867c6b2db6d"/>
		<rom name="stvbios.nv" size="128" crc="15432ae2" sha1="7d9364d546f3d3f839ec36be148076f8d26a65a6"/>
		<device_ref name="sh2_7604"/>
		<device_ref name="timer"/>
		<device_ref name="sh2_7604"/>
		<device_ref name="timer"/>
		<device_ref name="m68000"/>
		<device_ref name="sega_scu"/>
		<device_ref name="scudsp"/>
		<device_ref name="smpc_hle"/>
		<device_ref name="nvram"/>
		<device_ref name="93c46_16"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
		<device_ref name="gfxdecode"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="scsp"/>
		<device_ref name="segabill"/>
		<device_ref name="z80"/>
		<device_ref name="315_5338a"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="software_list"/>
	</machine>
	<machine name="su2000" sourcefile="misc/su2000.cpp" isbios="yes" runnable="no">
		<description>SU2000</description>
		<year>1993</year>
		<manufacturer>Virtuality</manufacturer>
		<rom name="amibios_486dx_isa_bios.u32" size="65536" crc="811d3639" sha1="a64d6026c16ac8c79f22b2c241f149402449fafb"/>
		<rom name="hmc86304_bios_v208.u7" size="32768" crc="c6c32f1a" sha1="a07ade7f0567e1978cd8cee73c6a5d7b5e5f947f"/>
		<rom name="u37 335d.u37" size="256" status="nodump"/>
		<rom name="u40 4116.u40" size="256" status="nodump"/>
		<rom name="ver_151_03_u16.u16" size="131072" crc="8354d059" sha1="a88df7cc259c1c39316cc3bff9e08aa4e8d3d2c0"/>
		<rom name="ver_151_03_u17.u17" size="131072" crc="ace4081d" sha1="f57287ded53f8d127bcdc9e34b8adb356fe55e5e"/>
		<rom name="wfc014a.u14" size="256" status="nodump"/>
		<rom name="wfc062_212.u62" size="32768" crc="9a6b553a" sha1="7045f733446866ee3171e175e1b22d9384fda1b5"/>
		<rom name="wfc065a.u65" size="256" status="nodump"/>
		<rom name="wfc066a.u66" size="256" status="nodump"/>
		<rom name="wfc067b.u67" size="256" status="nodump"/>
		<rom name="wfc071a.u71" size="256" status="nodump"/>
		<rom name="wfc072a.u72" size="256" status="nodump"/>
		<rom name="wi01p006.u6" size="2194" crc="528142eb" sha1="2c152c6540f3d38cb881296decba957f8b5c7c58"/>
		<rom name="wi01p025.u25" size="256" status="nodump"/>
		<rom name="wi01p026.u26" size="2194" crc="528142eb" sha1="2c152c6540f3d38cb881296decba957f8b5c7c58"/>
		<rom name="wi01p044.u44" size="2194" crc="a2ad9cf8" sha1="67d44807f7346baf87c15d35c27458b0a7d5de89"/>
		<rom name="wi01p045.u45" size="2194" crc="e2a13df7" sha1="eaa5ee3a92d11f0722934cb6d3443ead903dc78f"/>
		<rom name="wi01p046.u46" size="2194" crc="4c22fba5" sha1="6fabc7a0790f8b883b83fa6fe5f1ee1302d284e2"/>
		<rom name="wi01p047.u47" size="256" status="nodump"/>
		<rom name="wi01p048.u48" size="2706" crc="b9958131" sha1="058203eefb1645a446ff3ff4a170a673ad65076c"/>
		<rom name="wi01p049.u49" size="2706" crc="820d245a" sha1="8690e6eb46617c3dc78e1b233970a9318101101c"/>
		<rom name="wi01p050.u50" size="2194" crc="7cb0931f" sha1="394c100b33e5b8d1b2f4979399ad0791af39da28"/>
		<rom name="wi01p053.u53" size="2194" crc="d2eb2493" sha1="a66b4733da0f4f0869839630063c52a733f5ea8c"/>
		<rom name="wi01p054.u54" size="2194" crc="96d3506e" sha1="682ba8a7a17176ff41047cd9a9cfefdc2dc0fd64"/>
		<rom name="wi01p056.u56" size="2194" crc="8bf57db4" sha1="1a5315397b1903c36d7450e873603584db8a00e8"/>
		<rom name="wi01p058.u58" size="2194" crc="882f6405" sha1="e3b7c278f4ee9e0e11741d9ed7c5b32978a3d185"/>
		<rom name="wi01p067.u67" size="2194" crc="a97cff8e" sha1="78451a4bffecd4e1655e7a89971e28b47f5c8829"/>
		<rom name="wi01p070.u70" size="2706" crc="4322291e" sha1="e8751b585a4fb3f371e67616abf48c9d23847b77"/>
		<rom name="wi01p072.u72" size="2706" crc="fe77b66b" sha1="aa13619346a566613f0fa9e3723419f65ffd3ea8"/>
		<rom name="wi01p073.u73" size="2706" crc="e02fe7c1" sha1="ca22b30391453daae943007a0c04b5a28a958c18"/>
		<rom name="wi01p074.u74" size="2706" crc="fca2823c" sha1="6628f1ba3827a3d333ed88c5f20ca94a1439c75e"/>
		<rom name="wi01p075.u75" size="2194" crc="3d1adb17" sha1="b1af8c069de3df3c757e211b372f535b513c6326"/>
		<rom name="wi01p077.u77" size="256" status="nodump"/>
		<rom name="wi01p079.u79" size="2194" crc="3d3ad152" sha1="a769bc80514873c2f238e6c8842c5b23596b4a42"/>
		<rom name="wi01p080.u80" size="2194" crc="657a4495" sha1="c5bbd5e5f065a99f9f3d7ce89ca833779c338da5"/>
		<rom name="wi01p083.u83" size="2706" crc="902731aa" sha1="862c2e6fb75fbd712aeaf9eb3b8a84210332fa66"/>
		<rom name="wi01p087.u87" size="256" status="nodump"/>
		<rom name="wi01p092.u92" size="2706" crc="f996657e" sha1="01c2c774a9d5f4bcb78742cd606864eff512bfce"/>
		<rom name="wi02p000.u23" size="2706" crc="bab34c4b" sha1="a3f4f17a122cc0d063cb700b3d183b894d857cb4"/>
		<rom name="wi02p001.u32" size="2706" crc="b438ce94" sha1="f36c681b3d09835393a8be5079263915d3480b88"/>
		<rom name="wi02p002.u22" size="2706" crc="bab34c4b" sha1="a3f4f17a122cc0d063cb700b3d183b894d857cb4"/>
		<rom name="wi02p003.u31" size="2706" crc="b438ce94" sha1="f36c681b3d09835393a8be5079263915d3480b88"/>
		<rom name="wi02p004.u6" size="2706" crc="bab34c4b" sha1="a3f4f17a122cc0d063cb700b3d183b894d857cb4"/>
		<rom name="wi02p005.u14" size="2706" crc="b438ce94" sha1="f36c681b3d09835393a8be5079263915d3480b88"/>
		<rom name="wi02p006.u5" size="2706" crc="bab34c4b" sha1="a3f4f17a122cc0d063cb700b3d183b894d857cb4"/>
		<rom name="wi02p007.u13" size="2706" crc="b438ce94" sha1="f36c681b3d09835393a8be5079263915d3480b88"/>
		<rom name="wi02p008.u51" size="2194" crc="7c421890" sha1="49d0ab674a8cb4e18ae5ba570132111ed3ccd546"/>
		<rom name="wi02p009.u49" size="2194" crc="ff63d60c" sha1="8ee8629cc24cd18b944ffab3830ed474a1189179"/>
		<rom name="wi02p010.u72" size="2194" crc="68f48053" sha1="17ae9f5caa4b2f4ff700ce44294d3d2881bd4e62"/>
		<rom name="wi02p011.u88" size="2194" crc="78701d0f" sha1="089d5df945638cb811caa963430f5d6658c68947"/>
		<rom name="wi02p012.u85" size="2194" crc="1c489ff9" sha1="a0e1c00c9a5dd870b84f869070961d25724cea92"/>
		<rom name="wi02p013.u86" size="2194" crc="19de958f" sha1="a160f6b0e2a7e42457b470dbcf9415feaad880aa"/>
		<rom name="wi02p014.u82" size="2194" crc="845e4d48" sha1="6aaeabad0e86fe480773b4b51ca4f7c1c8935993"/>
		<rom name="wi02p015.u74" size="2194" crc="a10d1876" sha1="4091fa0a3abb2baeabcc6b250342cf29829af21a"/>
		<rom name="wi02p016.u52" size="2194" crc="d84b58c2" sha1="087b5a56ddb6bef6b1bc93b9a8e0d23de27aa399"/>
		<device_ref name="i486"/>
		<device_ref name="screen"/>
		<device_ref name="vga"/>
		<device_ref name="pic8259"/>
		<device_ref name="pic8259"/>
		<device_ref name="am9517a"/>
		<device_ref name="am9517a"/>
		<device_ref name="pit8254"/>
		<device_ref name="pit_counter"/>
		<device_ref name="pit_counter"/>
		<device_ref name="pit_counter"/>
		<device_ref name="ds12885"/>
		<device_ref name="kbdc8042"/>
		<device_ref name="at_keyb"/>
	</machine>
	<machine name="sys246" sourcefile="namco/namcops2.cpp" isbios="yes" runnable="no">
		<description>System 246 BIOS</description>
		<year>2001</year>
		<manufacturer>Namco</manufacturer>
		<rom name="r27v1602f.7d" size="2097152" crc="2b2e41a2" sha1="f0a74bbcaf801f3fd0b7002ebd0118564aae3528"/>
		<device_ref name="r5000le"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
	</machine>
	<machine name="sys256" sourcefile="namco/namcops2.cpp" isbios="yes" runnable="no">
		<description>System 256 BIOS</description>
		<year>2004</year>
		<manufacturer>Namco</manufacturer>
		<rom name="r27v1602f.8g" size="2097152" crc="b2a8eeb6" sha1="bc4fb4e1e53adbd92385f1726bd69663ff870f1e"/>
		<device_ref name="r5000le"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
	</machine>
	<machine name="sys573" sourcefile="konami/ksys573.cpp" isbios="yes" runnable="no">
		<description>System 573 BIOS</description>
		<year>1997</year>
		<manufacturer>Konami</manufacturer>
		<biosset name="std" description="Standard"/>
		<biosset name="gchgchmp" description="Found on Gachagachamp"/>
		<biosset name="dsem2" description="Found on Dancing Stage Euro Mix 2"/>
		<rom name="700a01,gchgchmp.22g" size="524288" crc="39ebb0ca" sha1="9aab8c637dd2be84d79007e52f108abe92bf29dd"/>
		<rom name="700a01.22g" size="524288" crc="11812ef8" sha1="e1284add4aaddd5337bd7f4e27614460d52b5b48"/>
		<rom name="700b01.22g" size="524288" crc="6cf852af" sha1="a2421d0a494892c0e71003c96995ce8f945064dd"/>
		<rom name="h8a01.bin" size="64" crc="131e0359" sha1="967f66578ebc0cf6b044d71af09b59bce1f4a1d0"/>
		<rom name="h8b01.bin" size="64" crc="508b057d" sha1="779177e6312ef272483eeb64a5e84bbae6e301f2"/>
		<rom name="hd6473644h.18e" size="32768" status="nodump"/>
		<device_ref name="cxd8530cq"/>
		<device_ref name="psxirq"/>
		<device_ref name="psxdma"/>
		<device_ref name="psxmdec"/>
		<device_ref name="psxrcnt"/>
		<device_ref name="psxsio0"/>
		<device_ref name="psxsio1"/>
		<device_ref name="ram"/>
		<device_ref name="ata_interface"/>
		<device_ref name="ata_slot"/>
		<device_ref name="ata_slot"/>
		<device_ref name="k572cassslot"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="mbm29f016a"/>
		<device_ref name="pccard"/>
		<device_ref name="pccard"/>
		<device_ref name="address_map_bank"/>
		<device_ref name="cxd8561q"/>
		<device_ref name="screen"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="psxspu"/>
		<device_ref name="m48t58"/>
		<device_ref name="adc0834"/>
		<device_ref name="sys573_jvs_host"/>
	</machine>
	<machine name="taitotz" sourcefile="taito/taitotz.cpp" isbios="yes" runnable="no">
		<description>Type Zero BIOS</description>
		<year>1999</year>
		<manufacturer>Taito</manufacturer>
		<rom name="e68-04-1.ic5" size="524288" crc="c7c2dc6b" sha1="bf88c818166c285130c5c73d6982f009da26e143"/>
		<rom name="e68-05-1.ic6" size="524288" crc="6ad9b006" sha1="f05a0ae26b6abaeda9c7944aee96c72b08fff7a5"/>
		<device_ref name="ppc603e"/>
		<device_ref name="tmp95c063"/>
		<device_ref name="ata_interface"/>
		<device_ref name="ata_slot"/>
		<device_ref name="idehd"/>
		<device_ref name="harddisk_image"/>
		<device_ref name="ata_slot"/>
		<device_ref name="nvram"/>
		<device_ref name="screen"/>
	</machine>
	<machine name="tourvis" sourcefile="pce/tourvis.cpp" isbios="yes" runnable="no">
		<description>TourVisión (PC Engine bootleg)</description>
		<year>19??</year>
		<manufacturer>bootleg (TourVisión)</manufacturer>
		<biosset name="60" description="V4-60"/>
		<biosset name="55" description="V4-55"/>
		<biosset name="54" description="V4-54"/>
		<biosset name="53" description="V4-53"/>
		<biosset name="52" description="V4-52"/>
		<biosset name="51" description="V4-51"/>
		<biosset name="43" description="V4-43"/>
		<biosset name="42" description="V4-42"/>
		<biosset name="40" description="V4-40"/>
		<biosset name="20" description="VT-20"/>
		<biosset name="11" description="VT-11"/>
		<rom name="v4-40.ic29" size="32768" crc="ba6290cc" sha1="92b0e9f55791e892ec209de4fadd80faef370622"/>
		<rom name="v4-42.ic29" size="32768" crc="0372606d" sha1="8c6a63865b0b4951ea032725cf022d353115b93b"/>
		<rom name="v4-43.ic29" size="32768" crc="88da23f3" sha1="9d24faa116129783e55c7f79a4a08902a236d5a6"/>
		<rom name="v4-51.ic29" size="32768" crc="2de0b946" sha1="c13051453aff3a2329f18ebade75c69aa3b1c28d"/>
		<rom name="v4-52.ic29" size="32768" crc="ffd7b0fe" sha1="d1804865c91e925a01b05cf441e8458a3db23f50"/>
		<rom name="v4-53.ic29" size="32768" crc="bccb53c9" sha1="a27113d70cf348c7eafa39fc7a76f55f63723ad7"/>
		<rom name="v4-54.ic29" size="32768" crc="125e7a6e" sha1="6f03c49acaad4feb9c2187f84fc1cb5451d0eb2b"/>
		<rom name="v4-55.ic29" size="32768" crc="87cf66c1" sha1="d6b42137be7a07a0e299c2d922328a6a9a2b7b8f"/>
		<rom name="v4-60.ic29" size="32768" crc="1fd27e22" sha1="b103d365eac3fa447c2e9addddf6974b4403ed41"/>
		<rom name="vt_1.1.bin" size="32768" crc="27abbc36" sha1="881ea7802b9e241473bc8ced0472e0f1851c9886"/>
		<rom name="vt_2.0.bin" size="32768" crc="36012f88" sha1="5bd42fb51aa48ff65e704ea06a9181bb87ed2137"/>
		<device_ref name="h6280"/>
		<device_ref name="c6280"/>
		<device_ref name="i8085a"/>
		<device_ref name="screen"/>
		<device_ref name="huc6260"/>
		<device_ref name="huc6270"/>
		<device_ref name="i8155"/>
		<device_ref name="speaker"/>
		<device_ref name="speaker"/>
		<device_ref name="generic_cartslot"/>
		<device_ref name="software_list"/>
	</machine>
	<machine name="triforce" sourcefile="sega/triforce.cpp" isbios="yes" runnable="no">
		<description>Triforce BIOS</description>
		<year>2002</year>
		<manufacturer>Sega</manufacturer>
		<biosset name="bios0" description="Triforce BIOS"/>
		<rom name="triforce_bootrom.bin" size="2097152" crc="d1883221" sha1="c3cb7227e4dbc2af861e76d00cb59726105a2e4c"/>
		<device_ref name="ppc603"/>
		<device_ref name="screen"/>
		<device_ref name="palette"/>
	</machine>
	<machine name="v4bios" sourcefile="barcrest/mpu4vid.cpp" isbios="yes" runnable="no">
		<description>MPU4 Video Firmware</description>
		<year>199?</year>
		<manufacturer>Barcrest</manufacturer>
		<rom name="vid.p1" size="65536" crc="e996bc18" sha1="49798165640627eb31024319353da04380787b10"/>
		<device_ref name="mc6809"/>
		<device_ref name="timer"/>
		<device_ref name="msc1937"/>
		<device_ref name="ptm6840"/>
		<device_ref name="pia6821"/>
		<device_ref name="pia6821"/>
		<device_ref name="pia6821"/>
		<device_ref name="pia6821"/>
		<device_ref name="pia6821"/>
		<device_ref name="pia6821"/>
		<device_ref name="meters"/>
		<device_ref name="bacta_datalogger"/>
		<device_ref name="coin_hopper"/>
		<device_ref name="speaker"/>
		<device_ref name="dac"/>
		<device_ref name="nvram"/>
		<device_ref name="mc68681"/>
		<device_ref name="duart_channel"/>
		<device_ref name="duart_channel"/>
		<device_ref name="ay8913"/>
	</machine>
</datafile>
